User Guide: AWC plug-in version 3.10.0 for VST-APL

# Overview

In this section, we will show you basic steps to configure an AWC-SC (AWC-Smart Connect) wireless network in a quick tour style.

> Note

> > AWC-SC is supported with TQ5403, TQ5403e, and TQm5403 firmware version 6.0.1-1.x or later.
> > Note that AWC-SC using AT-TQ6602 requires firmware to be released in the future.

For simplicity, we assume that we are going to create the following network with:

- AT-TQ5403 wireless APs.
- One floor (3F).
- 5 APs, 1 Root AP and 4 Satellite APs.
  The satellite APs will connect to the single Root AP and will act as Terminator APs, which do not bridge the connection between the Root AP and others.
- In usual client service communication, a multi-channel VAP will be used.
  Channel Blanket Network will not be provided.

Table 1: Devices in the target network
Device Name | Node Name | IP Address | MAC Address | Role
--- | --- | --- | --- | ---
Wireless Controller application container | 192.168.1.250 |  | AWC Plug-in
AlliedWare Plus Layer 3 Switch | 192.168.1.1 |  | PoE+ power sourcing, DHCP/NTP server
TQ5403 | TQ5403-SC-1 | 192.168.1.230 | 00:00:5E:00:53:00 | Root AP (wired) Powered by PoE+
TQ5403-SC-2 | 192.168.1.231 | 00:00:5E:00:53:20 | Satellite AP (wired) Powered by AC Adapters
TQ5403-SC-3 | 192.168.1.232 | 00:00:5E:00:53:40 | Satellite AP (wireless) Powered by AC Adapters
TQ5403-SC-4 | 192.168.1.233 | 00:00:5E:00:53:60
TQ5403-SC-5 | 192.168.1.234 | 00:00:5E:00:53:80

Based on this, the following wireless network will be created.

Table 2: Planned Wireless Networks
Radio | VAP | AP Profile | SC Profile | Overview
--- | --- | --- | --- | ---
Radio 1 | VAP1 | ForStaff | - | Wireless network for empolyees
Radio 2 | VAP1 | Default-1 (default) | SC-Default-cVVGG | For SC Management
VAP2 | - | sc-initial-provisioning (default) | For bootstrapping factory default APs (Automatic setting)

When applying the AP Profile and SC Profile, if there are specific configuration items for either AP or SC Profiles, those items will be applied to the AP as they are. If there are conflicting configuration items between the Profiles, the settings of the SC Profile take precedence over the AP Profile.
Therefore, VAP "Default-1" set by default on Radio 2 in the AP Profile is not used, "SC-Default-cVVGG" set in the SC Profile overrides the VAP.
In addition, for the VAP2 of the radio band declared to be used in the SC Profile, the SSID "sc-initial-provisioning" set by default for the factory default AP connection is used.
This is the same SSID defined for each radio band of the factory default AP, and is used for listening to the beacon of the factory default AP.

> Note

> > In the radio band used by AWC-SC, the other VAPs will be disabled automatically.

04 Jul 2023 13:01