User Guide: AWC plug-in version 3.11.0 for VST-APL

# Recommended Settings for TQ5000/6000 Series

When designing a cell-based (non-blanket) or AWC-CB wireless LAN using TQ5403/5403e/6602/6602 GEN2/6702 GEN2 and TQm5403/6602 GEN2/6702 GEN2, the following settings are recommended to ensure a stable wireless network.
Default settings are recommended for setting items not listed in this table. These are only recommended values, and you may need to adjust the settings depending on your environment.

Table 1: Recommended Settings for TQ5000/6000 Series
Item Name | Options included in | Scope of setting | Cell-based | AWC-CB | Comment
--- | --- | --- | --- | --- | ---
TQ5403 TQm5043 TQ5403e | TQ6602 | TQ6602 GEN2 TQ6702 GEN2 | TQ5403 TQ5403e | TQ6602 | TQ6602 GEN2 TQ6702 GEN2
Management Group | Management Group | - | Registered APs per management group: 50 or less |
Neighbor Managed AP Detection | AWC Settings | Whole AP | Disable when AWC Auto calc is not used | Disable when AWC Auto calc is not used | Neighbor management AP detection does not work when AWC-CB is enabled. | Disable when AWC Auto calc is not used |
Airtime Fairness | AP Profile | Per Band | Disable (default) | Disable (required, default) |
Legacy Rate Sets | AP Profile | Per Band | Disable 1, 2Mbps for 2.4GHz | Disable 1, 2Mbps for 2.4GHz |
RTS Threshold | AP Profile | Per Band | 2347 (default) | 2347 (required, default) |
Band Steering | AP Profile | Whole AP | Disable (default) | Disable (required, default) |
NoAck | - | Per Band | Disable (default) | Enable (default) | Disable (default) | Disable (default) | Enable (default) | Disable (default) | If a AP that has been used as a standalone is added to the management, check the settings on the Web GUI of the AP itself (Settings > QoS) and change them to the defaults shown on the left.
APSD | AP Profile | Per Band | Disable (default) | Enable (default) | Disable (default) | Disable (default) | Enable (default) | Disable (default) |
Neighbor AP Detection | AP Profile | Per Band | Neighbor AP detection (including IDS/IPS) not used and AWC auto-calculation low precision or not used: Disabled | Neighbor AP detection (including IDS/IPS) is not used: Disabled | Disable (required) |
MU-MIMO | AP Profile | Per Band | - | Disable (default) | - | Not Supported, Disable (required, default) |
OFDMA | AP Profile | Per Band | - | Disable (default) | - | Not Supported, Disable (required, default) |
Management Frame Protection (MFP) | AP Profile/ CB Profile | Per VAP | Disable | Disable |
Broadcast Key Refresh Rate | AP Profile/ CB Profile | Per VAP | 0 (default) | Not Supported, 0 (required, default) |
RADIUS Accounting | AP Profile/ CB Profile | Per VAP | Disable (default) | Not Supported, Disable (required, default) |
Dynamic VLAN | AP Profile/ CB Profile | Per VAP | Disable | Disable (default) | Not Supported, Disable (required) | Standalone AP: Disabled by default AP Profile: Enabled by default CB Profile: Always disabled
Fast Roaming | AP Profile/ CB Profile | Per VAP | Disable (default) | Not Supported, Disable (required, default) | Disable (default) |
Inactivity Timer | AP Profile/ CB Profile | Per VAP | 300 (default) | Not Supported, 300 (required, default) | 300 (default) |
Duplicate AUTH received | AP Profile/ CB Profile | Per VAP | Ignore | - | Ignore | Ignore | - | Ignore | For TQ6602 GEN2/TQ6702 GEN2, selecting "Disconnect" in the CB profile works the same as selecting "Ignore".
Association Advertisement | AP Profile/ CB Profile | Per VAP (in the case of AWC-CB, all CB VAPs in the relevant radio band.) | Enable | Environment where consists from only a single VAP and roaming does not occur: Disabled Environment where consists from multiple VAPs: Enabled |
DTIM Period | AP Profile/ CB Profile | Per VAP | Normal: 1 (default) When expecting to reduce device battery consumption: 3 | Normal: 1 (default) When expecting to reduce device battery consumption: 3 |
Proxy ARP | AP Profile/ CB Profile | Per VAP (in the case of AWC-CB, all CB VAPs in the relevant radio band.) | Disable for data communication Enable for IP telephony system | Disable for data communication Enable for IP telephony system |
RSSI Threshold | CB Profile | All CB-VAPs | - | 30 |
Force Power Save Disabled | CB Profile | All CB-VAPs | Disable (default) | Disable (default) |

14 Dec 2023 11:07