User Guide: AWC plug-in version 3.5.0 for VST-APL

# Access Management Screen

Start and Stop Server
Start Server
Stop Server
Login and Logout

When the AWC Plug-in is running on VST-APL, you can start and stop the AWC Plug-in server on the VST-APL Management screen.
Refer to the VST-APL User Guide for further information.

## Start and Stop Server

This section covers the steps to start or stop the AWC Plug-in server.

> Note

> > After restarting the server, the AWC Plug-in shows the last retrieved Management Status for unreachable APs, which may not be up-to-date. Once the APs become reachable again, the latest status will be displayed.

### Start Server

1. Log in to the VST-APL configuration screen.
2. Click "Wireless Controller" on the left-hand menu.
3. Click the "Start" button on the right end of the row in the "Deployed Application" list.
4. The state becomes "Running", and the "Start" button changes into the "Stop" button.

### Stop Server

1. Log in to the VST-APL configuration screen.
2. Click "Wireless Controller" on the left-hand menu.
3. The "Wireless Controller" management screen will appear. Click the "Stop" button on the right end of each row in the "Deployed Application" List.
4. The "State" indicator changes to "Stopping". Wait for a minute until "State" changes to "Stopped".

## Login and Logout

To use the AWC Plug-in with Vista Manager EX, you have to register it on Vista Manager EX's "Plug-in Management" screen. Please refer to the Vista Manager EX User Guide for more details.
Please refer to the "Login to Vista Manager EX" section of the Vista Manager EX User Guide for information on how to login to Vista Manager EX.
Once the AWC Plug-in is registered, the AWC Plug-in menu appears on the Vista Manager EX Main Menu.

22 Apr 2021 15:29