User Guide: AWC plug-in version 3.5.0 for VST-APL

# System Setting

The System Setting page lets you see the AWC Plug-in version, factory-reset the plug-in, and configure system settings.

> Note

> > This page is only accessible by Administrator accounts.

◼ System Information

Table 1: System Information
Item Name | Description
--- | ---
Version Information | Shows the AWC Plug-in's version information.
License Information | Wireless AP: Shows the number of APs allowed by the wireless LAN controller license and the number of APs which are being managed by the AWC Plug-in. License count: Shows the number of APs which are allowed to be managed by the installed wireless LAN controller license. Registered/Configured APs: Shows the number of APs which have been added to the AWC Plug-in's management database. Licensed APs: Shows the number of APs which are being managed by the AWC Plug-in. Channel Blanket: Shows the number of APs allowed by the channel blanket license and the number of APs which are operating in the AWC Plug-in's channel blankets. License count: Shows the number of APs which are allowed to be managed by the installed channel blanket license. Registered/Configured APs: Shows the number of APs which have been added to the AWC Plug-in's channel blankets. Licensed APs: Shows the number of APs which are operating in the AWC Plug-in's channel blankets. Smart Connect: Shows the number of APs allowed by the Smart Connect license and the number of APs which are operating in the AWC Plug-in's Smart Connect networks. License count: Shows the number of APs which are allowed to be managed by the installed Smart Connect license. Registered/Configured APs: Shows the number of APs which have been added to the AWC Plug-in's Smart Connect networks. Licensed APs: Shows the number of APs which are operating in the AWC Plug-in's Smart Connect feature.

◼ System Setting

Table 2: System Setting
Item Name | Description
--- | ---
Database Setting
Maximum Memory Usage | Specify the maximum amount of system memory that can be used for the AWC Plug-in database. Note Changing the maximum memory amount is not supported in the AWC Plug-in for VST-APL. Use the default setting.
"Save" button | Save and apply configuration changes to the database.
IP Address Settings
External IP address for AWC plug-in | Set the external IP address to be used for communication between the AWC Plug-in and the wireless APs. The default is "127.0.0.1". Note To manage the wireless AP, set this value to be the same as the IP address of the AWC Plug-in server (the "Wireless Controller" application in the VST-APL configuration screen). After registering the AWC Plug-in and after assigning a new IP address to the AWC Plug-in server, be sure to change it to the same IP address as the AWC Plug-in server.
"Save" button | Saves the changes to the IP address settings in the operation.
Data Retention Period Setting
Associated Client History | Specify a retention period for associated client histories that are displayed on the Screen Reference > Wireless Monitoring > Floor Map screen. Don't Save: The AWC Plug-in does not retain associated client history. Clients are not shown on the Floor Map's client history screen. Set Retention Period: The AWC Plug-in retains associated client histories within the specified period. The range for the retention period can be from 1 to 31 days. Note When you change this setting, the associated client history is initialized. Note The Data Retention Period Setting can be set up to 31 days on the screen, but the operation with the period up to 14 days is supported.
Client Location Estimation History | Specify a retention period for client location estimation histories that are displayed on the Screen Reference > Wireless Monitoring > Floor Map screen. Don't Save: The AWC Plug-in does not retain estimated client location information. Clients are not shown on the Floor Map's associated client location estimation history screen. The device counter in the Floor Map Associated Client View will also not count the number of clients of which the locations are estimated. Set Retention Period: The AWC Plug-in retains client location estimation histories within the specified period. The range for the retention period can be from 1 to 31 days. Note When you change this setting, the client location estimation history will be initialized. Note The Data Retention Period Setting can be set up to 31 days on the screen, but the operation with the period up to 14 days is supported. Client Location Estimation is available on this version of the AWC Plug-in combined with TQ5403/5403e firmware version 6.0.1-1.x or later. Note When this feature is enabled, the maximum number of wireless APs that can have CB Profiles applied is 500 over the entire system.
IDS Report History | Specify a retention period for IDS reports that are displayed on the Screen Reference > Wireless Monitoring > IDS/IPS Report page. Save only latest: The AWC Plug-in only retains neighbor AP information that has been detected within the last day. Rogue APs are not shown in the Floor Map's Rogue AP View. Set Retention Period: The AWC Plug-in retains neighbor AP information that has been detected during the specified period. The range for the retention period can be from 1 to 31 days. Note When you change this setting, the IDS report information is initialized. Note The Data Retention Period Setting can be set up to 31 days on the screen, but the operation with the period up to 14 days is supported.
Network Map Setting
Wireless Client Update-Interval | Specify the refresh interval for associated clients that are displayed on the Vista Manager EX "Network Map" screen. Don't Update: The AWC Plug-in does not refresh client information automatically. Set Update Interval: The AWC Plug-in refreshes client information automatically. The range for refresh interval can be from 1 to 9999 minutes. The update interval for links between AWC-SC APs on the Network Map also depends on this setting. It is set to 1 minute by default.
"Save" button | Save and apply configuration changes to the network map.
Remote Monitor Setting
Polling Interval | Set the polling interval for the information of the wireless LAN controller specified on the Remote Monitor screen, with a value from 5 to 30 (minutes). The default is 5 (minutes).
Log Retention Period | Set the number of days to keep the logs retrieved from the wireless LAN controller specified on the Remote Monitor screen, using a value from 1 to 366. The default is 366 (days).
Log Viewable Period | Set the number of log days to be displayed on the Remote Monitor screen, using a value between 1 and 90 (days). The default is 30 (days).
"Save" button | Save and apply configuration changes to the Remote Monitor in the operation.
Permission Setting
AMF Security WebAPI | Note This item is not supported.

◼ System Maintenance

Table 3: System Maintenance
Item Name | Description
--- | ---
Clear Cache
"Delete" button | Clears the AWC Plug-in cache.
Tech Support
"Tech Support" button | Note This button is for the maintenance by our service staff. Do not click.
Backup
"Backup" button | Saves the current settings to an external file as a backup file.
Include Log Data | If checked, the backup file will include the log data. By default, this option is not checked.
Restore
"Restore" button | Restores the settings from a backup file saved as an external file.
Initialize
"Initialize" button | Initialize the AWC Plug-in's data, such as its configuration and various histories.

See Operation Reference > Plug-in System Data Management > Backup and Restore and Operation Reference > Plug-in System Data Management > Initialize AWC Plug-in System for instructions on backup, restoration and initialization operations.

22 Apr 2021 15:29