User Guide: AWC plug-in version 3.7.0 for VST-APL

# View AP Information

Wireless AP Status Detail
Wireless AP Detail

This section describes how to view AP information.

> Note

> > The status displayed for an unreachable AP is the status that was last collected.

## Wireless AP Status Detail

This page shows detailed information about an AP's operation.
The page can be accessed by the following methods:

- Select "Wireless Monitoring" > "AP Status" > "Detail" (magnifying glass icon) in the rightmost column of the target AP.
- Select "Wireless Monitoring" > "Floor Map" > a Floor Map > an AP icon
- Select "Wireless Configuration" > "AP Settings" > "Detail" (magnifying glass icon) in the rightmost column of the target AP > "Wireless AP Status Detail" at the top of the Content section.

Table 1: Wireless AP Status Detail
Item Name | Description
--- | ---
Top of the Content section
Wireless AP Name | Shows the AP name.
"Gear" icon | When you move your cursor over the "Gear" icon, "Get Technical Support Information" will pop up. Get Technical Support Information: The file for the technical support will be output. This file is intended for use in troubleshooting and other situations where it is necessary to check internal information, please consult with our technical staff when using this feature.
Basic Information
"Wireless AP Detail" button | Opens the "Wireless AP Detail" page. This page shows you the detailed configuration applied to the AP. Refer to Wireless AP Detail for more information.
Management Status | Shows the Management Status of the AP.
Config Status | Shows the configuration status of the AP.
AP Profile | Shows the AP Profile for the AP. Clicking the link takes you to the "AP Profile Details" screen.
IP Address | Shows the AP's IP address.
MAC Address | Shows the device's MAC address.
Management Group | Shows the Management Group to which the AP belongs.
Assigned Firmware | Shows a target model name and version of the assigned firmware file. Note This is not necessarily the same as the "Current Firmware".
Use AMF for AP Provisioning | Shows whether the AWC Plug-in uses AMF guest device information to identify the AP.
Network Name | Shows the AMF network name to which the guest device AP belongs when "Use AMF for AP Provisioning" is enabled.
Area Name | Shows the AMF area name to which the guest device AP belongs when "Use AMF for AP Provisioning" is enabled.
Node Name | Shows the AMF parent device name to which the guest device AP is connected when "Use AMF for AP Provisioning" is enabled.
Port # | Shows the port number on the AMF parent device that the guest device AP is connected to when "Use AMF for AP Provisioning" is enabled.
Model | Shows the device type of the AP.
Current Firmware | Shows the currently running firmware version of the AP. Note This is not necessarily the same as the "Assigned Firmware".
Serial Number | Shows the serial number of the AP. (TQ3200, TQ3400, TQ4400, TQ4400e, TQ4600 only)
System Uptime | Shows the uptime of the AP.
Floor Map image | Shows the configured floor map image.
Floor Map Name | Shows the name of the configured floor map. Clicking the link takes you to the Floor Map Detail page.
Wireless Information
Current Channel | Shows the channels used on Radio1, 2 and 3.
Tx Power | Shows the transmit powers of Radio1, 2 and 3.
Detected Channel | If a weather radar has been detected on a channel, shows that channel (TQ series only).
Time to be Available | Shows the time for the channel where rader is detected to be available again. (TQ series only)
Associated Client Information
VAP | Shows the VAP number.
SSID | Shows the SSID for the VAP.
Clients | Shows the number of clients in the VAP.
Total | Shows the total number of clients in all VAPs.
Statistics Information
Graph | Shows the difference between the received byte counts on the wired interface and the transmit byte counts on the wireless network.

## Wireless AP Detail

This page shows details of the configuration applied to the AP.
The page can be accessed by the following methods:

- Select "Wireless Configuration" > "AP Settings" > "Detail" (magnifying glass icon) (the rightmost column)
- Select "Wireless Monitoring" > "AP Status" > "Detail" (magnifying glass icon) (the rightmost column) > "Wireless AP Detail" (at the top of the page).

> Note

> > WDS Configuration is displayed only if you configured WDS on the AP-specific configuration page.
> > Display items in the TQ series differ between TQ2450, TQ3200, TQ3400, TQ3600, TQ4400, TQ4400e, and TQ4600 when compared with TQ1402, TQm1402, TQ5403, TQ5403e, TQm5403, and TQ6602.

Table 2: Wireless AP Details
Item Name | Description
--- | ---
Top of the Content section
Wireless AP Name | Shows the AP name.
Basic Information
"Wireless AP Status Detail" button | Moves to the "Wireless AP Status Detail" page. This page shows you the operational status of the AP in details. Refer to Wireless AP Status Details for more information.
"Edit" button | Opens the "Wireless AP Edit" dialog box.
Management Status | Shows the Management Status of the AP.
IP Address | Shows the AP's IP address.
MAC Address | Shows the device's MAC address.
Management Group | Shows the Management Group to which the AP belongs.
Assigned Firmware | Shows a target model name and version of the assigned firmware file. Note This is not necessarily the same as the current firmware. It may be different from the firmware that is currently running on the AP.
Use AMF for AP Provisioning | Shows whether the AWC Plug-in uses AMF guest device information to identify the AP.
Network Name | Shows the AMF network name to which the guest device AP belongs when "Use AMF for AP Provisioning" is enabled.
Area Name | Shows the AMF area name to which the guest device AP belongs when "Use AMF for AP Provisioning" is enabled.
Node Name | Shows the AMF parent device name to which the guest device AP is connected when "Use AMF for AP Provisioning" is enabled.
Port # | Shows the port number on the AMF parent device that the guest device AP is connected to when "Use AMF for AP Provisioning" is enabled.
Floor Map image | Shows the configured floor map image.
Floor Map Name | Shows the name of the configured floor map. Clicking the link takes you to the Floor Map Detail page.
Configuration Information
"Edit" button | Moves to the AP-specific Configuration page.
AP Profile | Shows the AP Profile for the AP. Clicking the link takes you to the "AP Profile Details" screen.
CB Profile | Shows the CB Profile for the AP. Clicking the link takes you to the "CB Profile Details" screen.
SC Profile | Shows the SC Profile for the AP. Clicking the link takes you to the "SC Profile Details" screen.
Emergency VAP | Shows whether the AP is using the emergency VAP when it's configured in the AP Profile.
Config Status | Shows the configuration status of the AP.
Username | Shows the username used to logon to the AP's management web interface.
Password | Shows the configuration status of the password used to logon to the AP's management web interface.
Wireless Configuration | Shows the configuration for each radio band. The displayed radio bands vary depending on the Profile Type of the AP profile. Tri[11ac Wave2], Tri[11ac Wave2] with External Antenna (indoor configuration) Radio 1: 2.4GHz Radio 2: 5GHz (W52/W53) Radio 3: 5GHz (W56) Tri[11ac Wave2] with External Antenna (outdoor configuration) Radio 1: 2.4GHz Radio 3: 5GHz (W56) Dual[11ax], Dual[11ac Wave2], Dual[11ac], Dual[11n], 11ac with External Antenna Radio 1: 2.4GHz Radio 2: 5GHz (W52/W53/W56) Single Radio 1: either 2.4GHz or 5GHz (W52)
Channel | Shows the configured channel.
Tx Power | Shows the configured transmit power.
WDS Mode | Shows the WDS configuration as either "Disable", "WDS Parent" (WDS Root AP) or "WDS Child" (WDS Satellite AP). Note This is only available for TQ1402, TQm1402, TQ5403, TQ5403e, TQm5403, and TQ6602.
AWC Tx Power Lower Limitation | Shows the minimum transmit power which can be configured by AWC functionality. This is in effect only when "Tx Power" is set to "Auto".
Stop Radio Transmission | When the radio is disabled, this item is shown as "Stop".
WDS Configuration
TQ2450, TQ3200, TQ3400, TQ3600, TQ4400, TQ4600, TQ4400e
WDS List | Shows a list of configured WDSs. You can view WDS parameters such as status (enabled/disabled), WDS interface, and security here.
Radio Transmission | Shows the status (Enabled/Disabled) of the WDS.
Radio Interface | Shows the radio band for use with the WDS. The displayed radio bands vary depending on the Profile Type of the AP profile. Dual[11ac], Dual[11n], 11ac with External Antenna Radio 1: 2.4GHz Radio 2: 5GHz (W52/W53/W56) Single Radio 1: either 2.4GHz or 5GHz (W52)
MAC Address | Shows the MAC address of the remote AP.
Security | Shows the security mechanism used for WDS connection. This is the security configured on the AP-specific configuration page's WDS Configuration section. When the security is "Static WEP", the following items are also displayed. Key Length: the WEP key length. Key Type: the WEP key generation method. Security Key (WEP Key): The WEP key is shown by asterisks. Clicking the "Eye" icon reveals the key string. Clicking it again returns the key string to asterisks. When the security is "WPA Personal", the following items are also displayed. SSID: The SSID (Network name) used for the WDS connection. Security Key (WPA-PSK): The pre-shared key for the WDS connection is shown by asterisks. Clicking the "Eye" icon reveals the key string. Clicking it again returns the key string to asterisks.
TQ1402, TQm1402, TQ5403, TQ5403e, TQm5403, TQ6602
WDS List | Shows a list of configured WDSs. You can view WDS parameters such as status (enabled/disabled), WDS interface, and security here.
Radio Transmission | Shows the status (Enabled/Disabled) of the WDS.
Radio Interface | Shows the radio band for use with the WDS. Radio 1: 2.4GHz Radio 2: 5GHz (W52/W53) Radio 3: 5GHz (W56)
WDS Mode | Shows the AP's WDS mode (role) as either "WDS Parent" (WDS Root AP) or "WDS Child" (WDS Satellite AP).
SSID | Shows the SSID (Network name) used for the WDS connection.
Security | Shows the security mechanism used for WDS connection. This is the security configured on the AP-specific configuration page's WDS Configuration section. When the security is "WPA Personal", the following items are also displayed. Security Key (WPA-PSK): The pre-shared key for the WDS connection is shown by asterisks. Clicking the "Eye" icon reveals the key string. Clicking it again returns the key string to asterisks. WPA Version: The WPA version used for the WDS connection. Either "WPA2" or "WPA2, WPA" Encryption Protocol: The encryption protocol used for the WDS connection. Either "CCMP" or "CCMP, TKIP". Management Frame Protection: Shows whether to use Management Frame Protection. Either "Enable" or "Disable". Broadcast Key Refresh Interval: Shows the interval to refresh the broadcast key that is sent to clients on the VAP.

02 Nov 2021 15:51