User Guide: AWC plug-in version 3.11.0 for VST-VRT

# Manage Tags

Use Tags on Floor Map

You can tag various objects in the AWC Plug-in to make filtering easier.
This section describes how to add and delete tags on floor maps. The technique is the same on other pages.

## Use Tags on Floor Map

1. Select "Wireless Monitoring" > "Floor Map" from the AWC Plug-in menu.
2. Click the "List View" button at the top right of the Content section to show the floor maps in list view.
3. Check the floor maps on which you want to set or unset tags.
4. Click the "Tag" button at the top right of the Content section.
5. The "Set/Unset Tag" dialog box will appear.
6. Enter a tag of your choice and press the Enter key.
   A tag can contain up to 100 characters, but cannot contain successive spaces.
   A single map can contain 20 tags.

   > Note

   > > If you paste a tag string from the clipboard, not all text may be visible. In that case, press Enter to make a tag from the entire pasted string.

   > Note

   > > Pasting a tag containing a newline is not supported. It can result in a corrupted tag.

   > Note

   > > Tag names may be truncated in the tag filter list on the Devices Map, Floor Map Details and Device Search pages. To avoid this, use shorter names for the tags.

7. To delete a tag, click "x" to the right of the tag.
8. Click the "Save" button to save the changes.

14 Dec 2023 11:12