User Guide: AWC plug-in version 3.12.0 for VST-VRT

# Device Search

> Note

> > In this section, TQ4400 and TQ4600 are in Group A; TQ1402, TQ5403, TQ5403e, TQm1402, and TQm5403 are in Group B; and TQ6403 GEN2, TQ6602, TQ6602 GEN2, TQ6702 GEN2, TQ6702e GEN2, TQ7403, TQm6403 GEN2, TQm6602 GEN2, and TQm6702 GEN2 are in Group C.

> Note

> > TQ6702 GEN2-R allows users to configure VAPs and other settings via the CLI or web management screen of the wireless AP itself. The AWC Plug-in only checks radio and VAP settings and monitors wireless APs and Associated clients via a floor map. You can make changes to the settings on the AWC Plug-in, but you cannot apply them to the wireless APs. This table shows the availability of settings and operations from AWC Plug-ins, not of configuration from its CLI or Web GUI.

Table 1
Item Name | TQ | SDN TQ | Comment
--- | --- | --- | ---
Group A | Group B | Group C | TQ-R | Group A
4600 | 1402/ m1402 | 5403/ m5403 | 5403e | 6403 GEN2/ m6403 GEN2 | 6602 | 6602 GEN2/ m6602 GEN2 6702 GEN2/ m6702 GEN2 | 6702e GEN2 | 7403 | 6702 GEN2-R | 4400/ 4600
Export CSV File | Y | Y | Y | Y | Y | Y | Y | Y | Y | Y | Y |
Device Name | Y | Y | Y | Y | Y | Y | Y | Y | Y | Y | Y |
Model | Y | Y | Y | Y | Y | Y | Y | Y | Y | Y | Y |
Management Group | Y | Y | Y | Y | Y | Y | Y | Y | Y | Y | Y |
Firmware | Y | Y | Y | Y | Y | Y | Y | Y | Y | Y | Y |
IP Address | Y | Y | Y | Y | Y | Y | Y | Y | Y | Y | Y |
MAC Address | Y | Y | Y | Y | Y | Y | Y | Y | Y | Y | Y |
Details | Y | Y | Y | Y | Y | Y | Y | Y | Y | Y | Y |
Tag | Y | Y | Y | Y | Y | Y | Y | Y | Y | Y | Y |

12 Jul 2024 09:32