User Guide: AWC plug-in version 3.12.0 for VST-VRT

# Configure TQ6702 GEN2-R via CLI

Login
Wireless Configuration
Router Configuration
AMF Configuration
Save the Configuration
Configuration Example

Configure settings on the TQ6702 GEN2-R (wireless AP router), such as creating AP profiles, bridges, firewalls, DHCP servers, AMF settings, etc., using the CLI.

## Login

1. Log in to the wireless AP router CLI with a privileged user account (user with privilege level 15).
2. Shift to Privileged EXEC mode.

       awplus> enable
       awplus#

3. Shift from Privileged EXEC mode to Global Configuration mode.

       awplus# configure  terminal
       Enter configuration commands, one per line.  End with CNTL/Z.
       awplus(config)#

   * The prompts and command responses are omitted hereafter.

## Wireless Configuration

1. To configure the wireless function, type wireless command and shift to Wireless Configuration mode.

       wireless

2. Create security settings to be used for each VAP.
   - Set security mode to WPA Personal (security mode wpa-personal)
   - Set security key (key)
   - Specify WPA versions (versions)

       security 1 mode wpa-personal
        key passphrase1
        versions wpa2 wpa3
       security 2 mode wpa-personal
        key passphrase2
        versions wpa2 wpa3

3. Create network settings to be used for each VAP.
   - Network setting (network)
   - SSID name (ssid)
   - Enable SSID Stealth mode (hide-ssid)
   - Enable band steering (band-steering)
   - Selecting security profile (security)

       network 1
        ssid Network
        hide-ssid
        band-steering
        security 1
       network 2
        ssid Management
        hide-ssid
        band-steering
        security 2
       network 17
        ssid Network
        hide-ssid
        band-steering
        security 1
       network 18
        ssid Management
        hide-ssid
        band-steering
        security 2

4. Create a AP profile that configures various functions and VAPs for Radio 1/2.
   Use the "ap-profile local" command to enter AP Profile mode, then use the "radio" command to specify the radio number and execute the following command.
   - Enable the radio band (enable)
   - Enter VAP Configuration mode (vap)
   - Enable Zero Wait DFS (zero-wait-dfs enable)

       ap-profile local
        radio 1
         enable
         vap 0 network 1
         vap 1 network 2
        radio 2
         enable
         zero-wait-dfs enable
         vap 0 network 17
         vap 1 network 18

5. Once here, switch to Privileged EXEC mode and execute the "wireless ap-configuration apply ap local" command to apply the wireless configuration.
   This enables each VAP interface (vap1.0, vap1.1, vap2.0, vap2.1).
   After the wireless application is finished, return to the Global Config mode again to continue the configuration.

       end
       wireless ap-configuration apply ap local
       configure terminal

6. Create the software bridge 1 and 2. To do this, use the "bridge" command.

       bridge 1
       bridge 2

7. Assign vap1.0 and vap2.0 to bridge "1", and vap1.1 and vap2.1 to bridge "2". To do this, use the "bridge-group" command.

   > Note

   > > In this quick tour, 2.4GHz and 5GHz VAPs with the same VAP numbers belong to the bridges and operate in the same segments.
   > > When operating 2.4GHz and 5GHz VAPs in different segments, set IP addresses for each VAP and change entity and firewall settings.

       interface vap1.0
        bridge-group 1
       interface vap1.1
        bridge-group 2
       interface vap2.0
        bridge-group 1
       interface vap2.1
        bridge-group 2

8. Once again here, switch to Privileged EXEC mode and execute the "wireless ap-configuration apply ap local" command to apply the wireless configuration.
   If bridges are created after the VAPs are created and applied to the VAP, wireless application is required after the bridges are created.
   After the wireless application is finished, return to the Global Config mode again to continue the configuration.

       end
       wireless ap-configuration apply ap local
       configure terminal

## Router Configuration

1. Set IP addresses for Bridge 1 (br1) and Bridge 2 (br2) on separate segments. To do this, use the "ip address" command.

       interface br1
        ip address 192.168.10.1/24
       interface br2
        ip address 192.168.100.1/24

2. In the same way, set the IP address and netmask notified by the administrator of AMF Network to cpper port eth1.

       interface eth1
        ip address 192.168.1.200/24

3. Define "Entities" to be used when creating firewall and NAT rules.
   Create a zone "private" representing the internal network.
   To do this, use the "zone", "network", and "ip subnet" commands.

       zone private
        network dhcp
         ip subnet 0.0.0.0/0 interface br1
         ip subnet 0.0.0.0/0 interface br2
        network lan1
         ip subnet 192.168.10.0/24
        network lan2
         ip subnet 192.168.100.0/24

4. Create a zone "public" representing the external network.
   In addition to the above commands, the "host" and "ip address" commands are also used here.

       zone public
        network wan
         ip subnet 0.0.0.0/0 interface eth1
         host eth1
          ip address 192.168.1.200

5. Define the "Application" used to specify communication content when creating firewall rules.
   To do this, use the "application", "protocol", and "dport" commands.
   Define a custom application "DHCP" representing the DHCP packets.

       application dhcp
        protocol udp
        dport 67 to 68

6. Configure the firewall function to allow communication from outside to the wireless router while blocking communication between each bridge.
   To do this, use the "firewall", "rule", and "protect" commands.
   - Rule 10 - Allow internal DHCP communication
   - Rule 20 - Allow communication between terminals under bridge 1 and the wireless router
   - Rule 30 - Allow communication between terminals under bridge 2 and the wireless router
   - Rule 40 - Allow external communication from terminals under bridge 1
   - Rule 50 - Allow external communication from terminals under bridge 2
   - Rule 60 - Allow communication from the wired LAN interface of the wireless router to the outside
   - Rule 70 - Allow communication from the outside to the wired LAN interface of the wireless router.

       firewall
        rule 10 permit dhcp from private.dhcp to private.dhcp
        rule 20 permit any from private.lan1 to private.lan1
        rule 30 permit any from private.lan2 to private.lan2
        rule 40 permit any from private.lan1 to public
        rule 50 permit any from private.lan2 to public
        rule 60 permit any from public.wan.eth1 to public.wan
        rule 70 permit any from public.wan to public.wan.eth1
        protect

7. Configure the dynamic ENAT feature so that all terminals associated to the wireless LAN networks can use it.
   To do this, use the "nat", "rule", and "enable" commands.

       nat
        rule 10 masq any from private to public
        enable

8. Configure the DHCP server function for computers to be associated to the wireless LAN networks.
   To do this, create a DHCP pool with the "ip dhcp pool" command and set the following information:
   - Subnet (network)
   - IP address range to be leased (range)
   - Default gateway (default-router)
   - DNS server address (dns-server)
   - Lease time (lease)

       ip dhcp pool pool10
        network 192.168.10.0 255.255.255.0
        range 192.168.10.100 192.168.10.131
        dns-server 192.168.10.1
        default-router 192.168.10.1
        lease 0 2 0
       ip dhcp pool pool100
        network 192.168.100.0 255.255.255.0
        range 192.168.100.100 192.168.100.131
        dns-server 192.168.100.1
        default-router 192.168.100.1
        lease 0 2 0

9. Enable DHCP server. To do this, use the "service dhcp-server" command.

       service dhcp-server

10. Direct the default route to the default gateway notified by the administrator. To do this, use the "ip route" command.

        ip route 0.0.0.0/0 192.168.1.1

## AMF Configuration

1. Specify the AMF network name "AMF001".

       atmf network-name AMF001

2. Create an AMF virtual link to connect to the AMF master.

       atmf virtual-link id 1 ip 192.168.1.200 remote-id 1 remote-ip 192.168.1.254

   When the AMF virtual link is correctly communicated with the AMF master, the AMF network participation logs are displayed.
3. This completes the configuration of the wireless router.

       end

## Save the Configuration

After configuration is complete, save the current settings as a startup configuration. To do this, execute the copy command in the format "copy running-config startup-config".

    awplus# copy running-config startup-config
    Building configuration...
    [OK]

The same can also be done with the "write file" and "write memory" commands.

    awplus# write memory
    Building configuration...
    [OK]

## Configuration Example

The following is an example of a configuration set up in this quick tour.

    !
    wireless
     security 1 mode wpa-personal
      key passphrase1
      versions wpa2 wpa3
     security 2 mode wpa-personal
      key passphrase2
      wersions wpa2 wpa3
     network 1
      ssid Network
      hide-ssid
      band-steering
      security 1
     network 2
      ssid Management
      hide-ssid
      band-steering
      security 2
     network 17
      ssid Network
      hide-ssid
      band-steering
      security 1
     network 18
      ssid Management
      hide-ssid
      band-steering
      security 2
     ap-profile local
      radio 1
       enable
       vap 0 network 1
       vap 1 network 2
      radio 2
       enable
       zero-wait-dfs enable
       vap 0 network 17
       vap 1 network 18
     ap local
    !
    bridge 1
    bridge 2
    !
    interface vap1.0
     bridge-group 1
    !
    interface vap1.1
     bridge-group 2
    !
    interface vap2.0
     bridge-group 1
    !
    interface vap2.1
     bridge-group 2
    !
    interface br1
     ip address 192.168.10.1/24
    !
    interface br2
     ip address 192.168.100.1/24
    !
    interface eth1
     ip address 192.168.1.200/24
    !
    zone private
     network dhcp
      ip subnet 0.0.0.0/0 interface br1
      ip subnet 0.0.0.0/0 interface br2
     network lan1
      ip subnet 192.168.10.0/24
     network lan2
      ip subnet 192.168.100.0/24
    !
    zone public
     network wan
      ip subnet 0.0.0.0/0 interface eth1
      host eth1
       ip address 192.168.1.200
    !
    application dhcp
     protocol udp
     dport 67 to 68
    !
    firewall
     rule 10 permit dhcp from private.dhcp to private.dhcp
     rule 20 permit any from private.lan1 to private.lan1
     rule 30 permit any from private.lan2 to private.lan2
     rule 40 permit any from private.lan1 to public
     rule 50 permit any from private.lan2 to public
     rule 60 permit any from public.wan.eth1 to public.wan
     rule 70 permit any from public.wan to public.wan.eth1
     protect
    !
    nat
     rule 10 masq any from private to public
     enable
    !
    ip dhcp pool pool10
     network 192.168.10.0 255.255.255.0
     range 192.168.10.100 192.168.10.131
     dns-server 192.168.10.1
     default-router 192.168.10.1
     lease 0 2 0
    ip dhcp pool pool100
     network 192.168.100.0 255.255.255.0
     range 192.168.100.100 192.168.100.131
     dns-server 192.168.100.1
     default-router 192.168.100.1
     lease 0 2 0
    !
    service dhcp-server
    !
    ip route 0.0.0.0/0 192.168.1.1
    !
    atmf network-name AMF001
    !
    atmf virtual-link id 1 ip 192.168.1.200 remote-id 1 remote-ip 192.168.1.254
    end

12 Jul 2024 09:32