User Guide: AWC plug-in version 3.15.0 for VST-VRT

# System Setting

The System Setting page lets you see the AWC Plug-in version, factory-reset the plug-in, and configure system settings.

> Note

> > This page is only accessible by Administrator accounts.

## System Info

Table 1: System Information
Item Name | Description
--- | ---
Version Information | Shows the AWC Plug-in's version information.
License Information | Wireless AP: Shows the number of APs allowed by the wireless LAN controller license and the number of APs which are being managed by the AWC Plug-in. License count: Shows the number of APs which are allowed to be managed by the installed wireless LAN controller license. Registered/Configured APs: Shows the number of APs which have been added to the AWC Plug-in's management database. Licensed APs: Shows the number of APs which are being managed by the AWC Plug-in. Channel Blanket: Shows the number of APs allowed by the channel blanket license and the number of APs that are operating in the AWC Plug-in's channel blankets. License count: Shows the number of APs which are allowed to be managed by the installed channel blanket license. Registered/Configured APs: Shows the number of APs which have been added to the AWC Plug-in's channel blankets. Licensed APs: Shows the number of APs which are operating in the AWC Plug-in's channel blankets. Smart Connect: Shows the number of APs allowed by the Smart Connect license and the number of APs which are operating in the AWC Plug-in's Smart Connect networks. License count: Shows the number of APs which are allowed to be managed by the installed Smart Connect license. Registered/Configured APs: Shows the number of APs which have been added to the AWC Plug-in's Smart Connect networks. Licensed APs: Shows the number of APs which are operating in the AWC Plug-in's Smart Connect feature. Note When updating licenses related to AWC Plug-ins, the number of manageable units for both the pre- and post-renewal licenses may be posted in duplicate. After the grace period of the license before renewal is over, it will be displayed correctly.

## System Settings

Table 2: System Setting
Item Name | Description
--- | ---
Database Setting
"Save" button | Save and apply configuration changes to the database.
Maximum Memory Usage | Specify the maximum amount of system memory that can be used for the AWC Plug-in database. Note Changing the maximum memory amount is not supported in the AWC Plug-in for VST-VRT. Use the default setting.
History Data Retention Period Setting
"Save" button | Save and apply configuration changes to the History Data Retention Period Setting in the operation.
Wireless Clients | Specify a retention period for associated client histories that are displayed on the Wireless Monitoring > Floor Map screen. Don't Set The AWC Plug-in does not retain associated client history. Clients are not shown on the Floor Map's client history screen. Set: The AWC Plug-in retains associated client histories within the specifed period. The range for the retention period can be from 1 to 90 days. When "Wireless Client" is configured to "Set", the additional "Maximum Number of Wireless Client Records" described below will be displayed. Note All wireless client history information is retained after this setting is changed. Note The History Data Retention Period Setting of Wireless Clients can be set up to 90 days on the screen, but we support operation up to 14 days. When Client Packet Analysis in the AP Profile is enabled, operation for up to 90 days is supported. Note that when the "Client Packet Analysis" function is enabled, there are limitations on the management functions available in the Vista Manager EX basic functions. For more information, please see Client Connection History Management and Client Packet Analysis under Overview > What is the AWC Plug-in. Note When you use Wireless Client History with the following wireless APs, please set the log severity of the wireless AP to "information(6)" or "debug(7)". If the log severity is set to higher (lesser value) than "notice(5)", this feature will not work. The default value of the log severity of these wireless APs is "information(6)". If the wireless APs are not configured for logging, this function can still operate. Affected AP models: TQ1402, TQm1402, TQ3403, TQm3403, TQ5403, TQm5403, TQ5403e, TQ6403 GEN2, TQm6403 GEN2, TQ6602, TQ6602 GEN2, TQm6602 GEN2, TQ6702 GEN2, TQm6702 GEN2, TQ7403, TQ7613 The log severity can be set in the severity of the Syslog client in the AP profile. If you want to use the Wireless Client History View with the log function of the Syslog Client disabled, please change "Syslog Client" to "Enable" and "Severity" to "6 : informational" in the AP profile (the Syslog server IP address/host name can be a fictitious address). Apply this AP profile to the AP, and then set "Syslog Client" to "Disable" in the AP profile and apply it again.
Maximum Number of Wireless Client Records | Specify the max retention number of wireles client Association / Disassociation / Failure logs with a value in the range from 1,000,000 to 100,000,000. The default is 10,000,000.
Client Location Estimation | Specify a retention period for location estimation histories of wireless clients and APs that are displayed on the Wireless Monitoring > Floor Map screen. Don't Set The AWC Plug-in does not retain estimated location information. Clients are not shown on the Floor Map's associated location estimation history screen. Device counter in the Floor Map Associated Client View also will not count the number of clients of which the locations are estimated. Set: The AWC Plug-in retains location estimation histories within the specifed period. The range for the retention period can be from 1 to 31 days. Note When this item is changed from "Don't set" to "Set", or vice versa, the Config Statuses of APs belonging to a Channel Blanket will become "Modified". Please apply the configuration to the AP from either the Wireless Monitoring > Floor Map Details [Wireless Status View], Wireless Configuration > CB Profile", or Wireless Configuration > AP Settings screen after changing the setting. Note When you change this setting, the Location Estimation History information will be initialized. Note The History Data Retention Period Setting can be set up to 31 days on the screen, but we support operation up to 14 days. Note Location Estimation is available on this version of the AWC Plug-in combined with TQ6602 GEN2/TQ6702 GEN2 firmware version 8.0.3-0.x or later, or TQ5403/TQ5403e firmware version 6.0.1-1.x or later. Note When this feature is enabled, the maximum number of wireless APs that can have CB Profiles applied is 500 over the entire system.
IDS Report | Set the duration of the history to be displayed on the Wireless Monitor > IDS/IPS Report screen. Save only Latest: The AWC Plug-in only retains neighbor AP information that has been detected within the last day. Saved by Specific Period The AWC Plug-in retains neighbor AP information that has been detected during the specifed period. The range for the retention period can be from 1 to 31 days. Note When you change this setting, the IDS report information is initialized. Note The History Data Retention Period Setting can be set up to 31 days on the screen, but we support operation up to 14 days.
Log | Can specify how long the AWC Plug-in logs are stored in the database. Don't Set No log storage period is set. If the number of logs is within the "Maximum Number of Logs" parameter, they will remain stored in the database regardless of the number of days elapsed since they were recorded. Set: Specify the log storage period with a value in the range 1-31 (unit: days). Logs whose number of days elapsed since recording exceeds the specification in this item are deleted. Note that logs that exceed the maximum number of logs, even within the retention period, will be deleted from the oldest logs. The default is "Don't Set". In addition, if "Set" is selected, the default retention period is 7 (days).
Maximum Number of Logs | Specifies the maximum number of Logs related to AWC Plug-in, from 10,000 to 5,000,000. If the number of logs recorded in the AWC plug-in database exceeds the value set in this item, the oldest logs are deleted first to keep the number within the value. The default is 5,000,000.
Datetime format in CSV files
"Save" button | Applies the change to the Datetime format in CSV files.
Datetime Format | Select the date/time format to be recorded in the CSV file. YYYY-MM-DDThh:mm:ssZ Represents UTC (Coordinated Universal Time) in the "YYYY-MM-DDThh:mm:ssZ" format based on ISO 8601. YYYY-MM-DD hh:mm:ss Represents the local date and time based on the selected time zone. The "Time Zone" is displayed additionally. The default is "YYYY-MM-DDThh:mm:ssZ".
Timezone | Describe the timezone as a region name and a city name (e.g. "(UTC+09:00) Asia/Tokyo"). The default is "Not Set". You can also narrow down the options displayed in the drop-down list by entering a part of the timezone character string in the search field above the drop-down list. Displayed only when the "YYYY-MM-DD hh:mm:ss" format is specified for "Datetime Format".
Network Map Setting
"Save" button | Save and apply configuration changes to the network map.
Wireless Device Topology Data Update-Interval | Specify the refresh interval for APs and wireless clients that are displayed on the Vista Manager EX "Network Map" screen. Don't Set The AWC Plug-in does not send wireless device information to the Vista Manager EX. In this case, the wireless devices managed by the AWC Plug-in don't appear on the Device list or the network map in the Vista Manager EX. The information of these devices are not checked against the registered device information on the Vista Manager EX, so custom icons on the Vista Manager EX will not reflected in the AWC Plug-in, and are displayed as default icons instead. Set: The AWC Plug-in refreshes wireless device information automatically. The wireless devices managed by the AWC Plug-in will be displayed in the Vista Manager EX. If a custom icon is applied in Vista Manager EX, it will also be reflected in the AWC Plug-in's floor map and other displays. Also, set the update interval with a value from 1 to 9999 (unit: minutes). Information on wireless devices and link lines between APs in the AWC-SC are reflected in the network map according to this update interval. It is set to 1 minute by default. When "Wireless Device Topology Data Update-Interval" is set to "Set", the following additional "Target Data" will be displayed.
Target Data | Select the target data for the information displayed on the "Network Map" screen of the Vista Manager EX from "AP and Associated Client" or "Only AP". The default is "AP and Associated Client". When "AP and Associated Client" is selected, information on the currently connected wireless client will be sent along with the AP's IP address, MAC address, management status, etc. If the relevant wireless client is registered in the Vista Manager EX, the custom icon of the registered wireless client on the Vista Manager EX will also be reflected in the AWC Plug-in's floor map. When "Only AP" is selected, only the IP address, MAC address, and management status of the wireless AP will be notified, and no information about the connected wireless clients will be sent. In this case, the custom icons of wireless clients registered on the Vista Manager EX will not be reflected in the AWC plug-in floor map, even if the corresponding wireless clients are registered in the Vista Manager EX.
Remote Monitor Setting
"Save" button | Save and apply configuration changes to the Remote Monitor in the operation.
Polling Interval | Set the polling interval of the wireless LAN controller specified on the Remote Monitor screen, with a value from 5 to 30 (minutes). The default is 5 (minutes).
Log Retention Period | Set the number of days to keep the logs retrieved from the wireless LAN controller specified on the Remote Monitor screen, using a value from 1 to 366. The default is 366 (days).
Log Viewable Period | Set the number of log days to be displayed on the Remote Monitor screen, using a value between 1 and 90 (days). The default is 30 (days).
VAS History Mode Setting
| Note AT-VST-VRT does not support VAS History Mode Setting.
Permission Setting
AMF Security WebAPI | Displays the sending IP address of the Web API used by our AMF-Security Controller AT-SecureEnterpriseSDN Controller (AT-SESC) and AMF Security mini. If multiple IP addresses are registered, they will be displayed separated by a slash (/). "Edit" button: Displays Permission Setting (AMF Security WebAPI) dialog box.

### Permission Setting (AMF Security WebAPI)

When the AMF Security server (AMF-Sec or AMF Security mini) receives a threat event, it queries the AWC plug-in for the MAC address from the IP address of the threat device via Web API.
Register the IP address of the AMF Security server that you want to allow access to in order to respond only to inquiries from legitimate AMF Security servers.
AMF Security Server IP addresses can be registered up to 1,024 entries.

Table 3: Permission Setting (AMF Security WebAPI) dialog box
Header
Permitted IP Address | Enter the IP address of the AMF Security server to grant access to.
"Add" button | Add the IP address to the list.
"Clear" button | Clear the Permitted IP address field.
IP Address list
X IP Address | Shows the number of IP address entries registered to the list.
Search IP address | Search for a particular IP address. Enter a partial string to match. The list shows entries with that string in the "IP Address" field. To remove the filter, delete the string from the search field and press enter.
IP Address | Displays registered IP address of the AMF Security server (AMF-Sec or AMF Security mini).
Delete (trashbin icon) | Deletes the entry of AMF Security server IP Address.
Footer
"Save" button | Save changes of the permission setting and close the dialog box.
"Exit" button | Discard changes of the permission setting and close the dialog box.

## System Maintenance

Table 4: System Maintenance
Item Name | Description
--- | ---
Clear Cache
"Delete" button | Clears the AWC Plug-in cache.
Tech Support
"Tech Support" button | Note This button is for maintenance purposes. For use by support staff only.
Backup
"Backup" button | Saves the current settings to an external file as a backup file.
Include in Backup File
Wireless Client History | If checked, the backup file will include the wireless client history. By default, this option is not checked.
Location Estimation History | If checked, the backup file will include the location estimation history. By default, this option is not checked.
Logs on Management Log Page | If checked, the backup file will include the log data in the Log Management screen. By default, this option is not checked.
Logs on Remote Monitor | If checked, the backup file will include the log data from Remote Monitor. By default, this option is not checked.
Restore
"Restore" button | Restores the settings from a backup file saved as an external file.
Restore System Setting | If checked, system settings are restored from a backup file, together with management information such as APs and floor maps. By default, this option is not checked. System Configuration includes the following: Database Setting Maximum Memory Usage History Data Retention Period Setting Wireless Clients Maximum Number of Wireless Client Records Client Location Estimation IDS Report Log Maximum Number of Logs Network Map Setting Wireless Device Topology Data Update-Interval Pointing the words "Restore System Setting" shows the items included in the above system settings in the pop-up balloon.
Initialize
"Initialize" button | Initialize the AWC Plug-in's data, such as its configuration and various histories.

For detailed procedures to backup, restore, or factory-reset the AWC Plug-in system, refer to Operation Reference > Plug-in System Data Management > Backup and Restore AWC Plug-in System> or Operation Reference > Plug-in System Data Management > Initialize AWC Plug-in System.

10 Nov 2025 11:49