User Guide: AWC plug-in version 3.15.0 for VST-VRT

# DCN Profile

The DCN Profile is a pile of settings that are commonly applied to the APs used in AWC-DCN (AWC-Dynamic Client Navigation), including configurations for communicating management information among the APs belonging to the DCN group, DCN VAPs, and other settings.
This page allows you to create, edit, and delete DCN profiles, and apply configurations to the APs selected as the targets of an DCN profile.

Section 1

Table 1
Item Name | Description
--- | ---
"Create" button | Shows the DCN Profile configuration screen. Refer to Operation Reference > AWC-DCN > Configure DCN Profile for more details.
"Apply Config" button | Opens the "Apply Configuration" dialog box. It allows you to apply changes to the selected SC profile to APs that have been assigned to the DCN profile. X AP: Shows the number of APs to which the DCN Profile is applied. Device Name: Shows the name of the AP. If the AP was added from the Guest Device List, the guest device name is displayed. IP Address: Shows the AP's IP address. MAC Address: Shows the device's MAC address. Management Status: Shows the Management Status of the AP. Unmanaged: The AP is not managed, because any of the IP address, MAC address, or AP profile is not configured. Configurations cannot be applied to unmanaged APs. Discovering: The AWC Plug-in is searching for the AP. Applying: The AWC Plug-in is applying a configuration update to the AP. Managed: The AP is being managed by the AWC Plug-in. Waiting: The AP was provisioned by AMF configuration and has just been assigned an AP Profile. Or, the AP was provisioned to use DHCP to register IP/MAC addresses to the AWC Plug-in, and has just been assigned an AP Profile. Failed: The AP is no longer managed by the AWC Plug-in. Not Authenticated: The AP cannot be managed because the number of managed APs reached the maximum number allowed by the registered Wireless AP licenses. Alternatively, the AP cannot be managed because the AP belongs to a Channel Blanket or Smart Connect network, but the number of managed APs has reached the maximum number allowed by the registered Channel Blanket / Smart Connect licenses. Config Status: Shows the configuration status of the AP. Not Configured: The AP is not fully configured. Not Applied: The configuration has not been applied to the AP by the AWC Plug-in. Latest: The latest configuration has been applied to the AP. Pending: An out-of-date configuration has been applied to the AP (newer configuration has not been applied). AP Profile: Shows the AP Profile assigned to the AP. "OK" button: Applies the changes of the settings, including DCN and other (AP, CB, and SC) profiles, to the AP. Note AWC-DCN is not supported mixed with AWC-SC or AWC-CB. If other kinds of profiles are applied at the same time, the SC profile, CB profile, DCN profile, and AP profile will take precedence in that order. It also applies pending AP-specific configuration updates to APs. "Cancel" button: Cancels applying configuration changes to the AP.

Section 2

Table 2: DCN Profile List
Item Name | Description
--- | ---
X DCN Profiles | Shows the number of DCN Profiles.
X SELECTED | Shows the number of selected DCN Profiles.
All ON/All OFF buttons | Turn all DCN profiles ON or OFF. To apply the changes, you must tick the checkbox for the target DCN profile and then "Apply Config".
Search DCN Profile | Lets you search and filter DCN Profiles in the list. The Search field lets you enter a partial string to match. The screen displays entries with that string in one of the following fields: "DCN Profile Name" or "Management Group". To remove the filter, delete the string from the search field and press enter. Note The search is case-sensitive.
DCN Profile List
Checkbox | Lets you select or deselect DCN Profiles. A checkbox in the header row can be used to check or uncheck all DCN Profiles. Unchecking the box in the heading row deselects all entries in the list.
DCN Profile Name | Shows the DCN Profile name.
Management Group | Shows the list of management groups for the DCN Profile.
Assigned APs | Shows the number of APs to which the DCN Profile is assigned.
Unapplied APs | Shows the number of APs, for which some pending configurations (AP Profile, CB Profile, SC Profile, DCN Profile or AP-specific configurations) exist, and which belong to the DCN group. Note AWC-DCN is not supported mixed with AWC-SC or AWC-CB.
DCN ON/OFF | Can select the radio button to enable (ON) or disable (OFF) the relevant DCN. To apply the changes, you must tick the checkbox for the target DCN profile and then "Apply Config".
Edit (pencil icon) | The DCN Profile configuration screen will appear. Refer to Operation Reference > AWC-DCN > Configure DCN Profile for more details.
Delete (trashbin icon) | Deletes the DCN Profile. Refer to Operation Reference > AWC-DCN > Configure DCN Profile for more details.
Details (magnifying glass icon) | The "DCN Profile Detail" page will appear. The items displayed on the DCN profile detail screen are almost the same as those on the edit screen. Refer to Operation Reference > AWC-DCN > Configure DCN Profile for descriptions.

Section 3

Table 3
Item Name | Description
--- | ---
Items per page | Specifies the number of items per page.
<< | Goes to the first page of the list.
(Page Number) | Shows the current page number in the list.
>> | Goes to the last page of the list.

10 Nov 2025 11:49