User Guide: AWC plug-in version 3.15.0 for VST-VRT

# Floor Map Detail [Wireless Status View]

Clicking on a floor map panel or selecting a specific floor map from the floor map dropdown menu will show the "Floor Map Details" page.
The floor map is displayed in the center of the Content section and a list of APs is shown on the right side of the Content section.

> Note

> > The status displayed for an unreachable AP is the status that was last collected.

> Note

> > If you try to move an AP icon, it may move to an unintended position and your mouse cursor and the icon may become out of sync.
> > If this occurs, release your mouse button and drag the icon again.

> Note

> > If you try to place an AP on a floor map that was deleted by another user, you will be brought back to the "Floor Map Details" page without any error message. In such cases, please check if the floor map still exists on the "Floor Map List" page.

## Wireless Status View

Displays wireless signal Comfort Level, Power (signal strength) and Channel on a floor map.
In the floor map control described below, you can switch between Comfort Level, Power, and Channel modes from the Drawing Mode drop-down menu.

### Common Items

The display items common to the Comfort Level, Power, and Channel modes are shown below.

Section 1

Table 1: Floor Map Header
Item Name | Description
--- | ---
Management Group / Floor Map Group | The floor map name and the management group of the selected floor map will be displayed.
"Spanner" icon | Hovering the mouse cursor over the Spanner icon shows a dropdown menu including some operations for managed APs. Select APs by checking on the AP list or clicking the AP icons on the floormap, you can then execute the following operation for the selected APs. Apply Configuration: Applies changes made on the "Configuration Mode" page to the selected APs. Reboot: Reboots the selected APs. Assign Firmware: Displays the "Select assign firmware" dialog box, which allows you to select a firmware file to be applied to the APs for the next time you execute the firmware update. Firmware file to be selected is supposed to be registered on the Firmware Registration screen in advance. Refer to Operation Reference > Miscellaneous Settings > Reboot AP and Update AP Firmware" > "Assign Firmware To AP for more details. The firmware file assigned to an AP can be reviewed in the Wireless AP Details or Wireless AP Status Details pages' under the Basic Information section. Upgrade Firmware: Opens the "Upgrade Firmware" dialog box. You can update the selected APs using firmware files that were assigned to each AP on running "Assign Firmware". Refer to Reboot AP and Update AP Firmware" > "Update Firmware for more details. Note A single floor map supports a maximum of 120 APs. According to this, the number of APs which can be updated in a single operation is up to 120. Depending on the conditions of the transmission speed between the AWC plug-in and each wireless AP and the band usage, the number may be less than the above. AWC Calculate and Apply: Perform AWC calculation and apply the results to all APs in the Management Group which the current floor map belongs to. Save Floor Map Display Settings: The current floor map display and selected options are saved as shared settings for all users. The following options are saved. Radio dropdown menu View Selection dropdown menu Drawing Mode drop-down menu Grid checkbox AP Name checkbox Legend checkbox Details checkbox Healthiness Icon checkbox Floor Area checkbox Device Counter checkbox Wall checkbox Power Limit slider Background Opacity slider Floor Map display position Floor Map zoom rate Note Other floor maps are not affected. Note Changes cannot be reverted to the initial states. It is necessary to manually adjust the drawing settings to an equivalent display position and magnification to the initial states and re-save the drawing settings, or re-create the floor map.
Radio dropdown menu | Lets you select a radio band to show on the map from following options: Radio 1 - 2.4GHz Radio 2 - 5GHz Radio 3 - 5GHz Radio 3 - 6GHz "Radio 3 - 5GHz" corresponds to TQ5403, TQ5403e, TQm5403, TQ6403 and TQm6403 Radio 3, and "Radio 3 - 6GHz" corresponds to TQ3403, TQm3403, TQ7403, and TQ7613 Radio 3.
View Selection dropdown menu | Lets you change what information is displayed on the Floor Map Details screen. Wireless Status View Wireless Client Smart Connect View Rogue AP View Add AP to Map Edit Area Edit Wall
"Back to list" button | Click to return to the Floor Map List screen.

Section 2

In Wireless Status View, the "Healthiness Icon" is disabled.

Table 2: Floor Map Control
Item Name | Description
--- | ---
Drawing Mode | Lets you select what to show on the heatmap. Options are Comfort Level, Power (signal strength) and Channel. The default is "Comfort Level".
Grid | Lets you enable or disable grid lines on the floor map. Checking this shows grid lines on the floor map.
Wireless AP Name | Whether to display the AP name above the AP icon. Check to display.
Legend | Lets you enable or disable the legend. Check to display.
Details | Whether to display the list of placed APs. Check to display.
Floor Area | If areas have been created on the floor map (using the Edit Area page), this lets you choose whether to display the areas. Check to display.
Device Counter | On the top left of an area, indicates the number of registered APs that are arranged in the area.
Wall | Lets you choose whether to display the walls if walls have been created on the floor map (using the Edit Wall page). Check to display. Note If walls have been defined, attenuation by the walls takes effect over the heat map even if this control is left unchecked.
Power Limit | Specify the minimum signal strength to show in colors on the heatmap. Disabled in comfort level mode.
Opacity | Specify the opacity of the floor map background image.

Section 3

Zoom In/Out buttons.
You can zoom in (+) or zoom out (-) of the floor map display. You can also use the mouse wheel scroll to zoom in or out.

### Comfort Level Mode

The floor is color-coded by comfort level, based on five comfort parameters: Channel Availability, Client Capacity, Connection Stability, Wi-Fi signal stability, and Airtime Capacity.

Section 1

Displays numerical values (in %) and graphs of the comfort level of the entire floor, as independently calculated by AWC Plug-in.
Clicking on any point on the floor map switches to a display of the comfort level at that point.

Section 2

Table 3: Floor Map
Item Name | Description
--- | ---
Floor Map (Background) | The map image specified when you created the map is shown. You can place icons for the APs in the righthand-side list. In addition, heat map is drawn with colors representing the reach and strength of the channel or signal. The drawing mode of the heat map can be selected from the floor map control. Note Even between wireless APs operating at the same radio strength, the size of output circle on the heat map may vary depending on the installation location and other factors. If the AP is not managed by the AWC Plug-in, does not affect the floor map.
Wireless AP Icon | AP icons placed on the map is shown. If "AP Name" is checked in the floor map controls, the AP name is displayed above the AP icon. The current status is displayed under the icon of the AP under the AWC Plug-in management. Radio signals being output in the selected radio band: Simplified display of current status depending on whether a connected wireless client is present. When one or more wireless clients are connected to the AP: In the format "[current channel]ch([radio usage]%), [radio strength]%, [number of clients] client(s)" (For example, "7ch(50%), 100%, 2 clients") When no wireless client is connected to the AP: In the format "[current channel]ch([radio usage]%), [radio strength]%" (For example, "7ch(50%), 100%") When Wireless Concierge AP Thinning is enabled and the AP in question is subject to thinning: Shown as "Standby". The AP in question is not providing radio output in the radio band being displayed. If the radio transmission is stopped by the Wireless AP Individual Configuration: Shown as "Stop". The AP in question is not providing radio output in the radio band being displayed. When you place your mouse cursor on an AP, the management information of the AP will pop up. Wireless AP Name MAC Address IP Address Used channels, bandwidth, and output strength of the currently displayed radio band. Number of Clients Last failed at (date and time last out of control)
Rogue AP Icon | If Unmanaged AP Detection is enabled, this represents the estimated location of the unmanaged APs that are particularly impacting. When you hover the mouse pointer over the icon, the SSID, BSSID, channel, radio strength (RSSI), and detection time sent out by the concerned unmanaged AP will pop up.

Section 3

Shows the heatmap legend.
It shows the relationship between colors and comfort level.
The legend can be made invisible or visible by using a checkbox in the floor map control section at the bottom of the page.

Section 4

Table 4: Floor Map Comfort Parameters Details
Item Name | Description
--- | ---
Details | Disabled in comfort level mode.
X AP | Shows the number of APs placed on the floor map.
Refresh Timer | Shows the status of the timer that automatically refreshes the page with the blue progress bar. The list is automatically refreshed at the interval configured on "Refresh Rates" > "Floor MAP (Wireless Status)" in the User Management menu. (The default is 1 minute.) You can also specify whether to pause or resume automatic updates by clicking Resume/Pause automatic update button on the right, or force the list to be updated by clicking the Manual update button.
Comfort Parameters chart | The following five comfort parameters are displayed as a radar chart. Channel Availability: Magnitude of impact of radio frequency interference with unmanaged APs. Higher value indicates less interference from unmanaged APs. Note In order to properly display this parameter, "Rogue AP Detection" in the Wireless IDS/IPS Settings and "Neighbor AP Detection" in the AP profile must be set to enabled. Client Capability: Degree of allowance for wireless client associates. Higher value indicates fewer current client connections relative to the maximum number of client connections. Connection Stability: Degree of low anomaly logs among the received wireless associate logs. Higher value indicates less wireless connection problems. Wifi Signal Stability: Optimal degree of AP placement, signal output, and channel settings. Higher value indicates proper placement and configuration of APs. Airtime Capacity: Degree of airtime utilization. Higher value indicates less communication relative to the radio communication bandwidth. The color of the entire graph indicates the comfort level of the entire floor or, when a specific location is clicked, the comfort level of the specified location. By clicking on each parameter in the graph, you can exclude or re-include the relevant parameter from evaluation in the heat-map display. The parameter name excluded from evaluation is grayed out. If the comfort level is low, hover the mouse pointer over the caution icon on the left side of the title to see suggestions for improvement.
Rogue BSSIDs Distribution | Displays the radio waves of rogue APs emitted by wireless devices other than managed APs detected by the APs on the floor map in the past hour as channels on the horizontal axis and output strength (RSSI) on the vertical axis. Click on the graph to enlarge. Note In order to view this graph, "Rogue AP Detection" in the Wireless IDS/IPS Settings and "Neighbor AP Detection" in the AP profile must be set to enabled.
Wireless Connection Logs | Displays the number of success logs such as associations, failure logs such as disconnections, and information logs such as channel blanket handovers of wireless clients to the APs on the floor map over the past hour.

### Signal Power Mode

Section 1

Table 5: Floor Map
Item Name | Description
--- | ---
Floor Map (Background) | The map image specified when you created the map is shown. You can place icons for the APs in the righthand-side list. In addition, heat map is drawn with colors representing the reach and strength of the channel or signal. The drawing mode of the heat map can be selected from the floor map control. Note Even between wireless APs operating at the same radio strength, the size of output circle on the heat map may vary depending on the installation location and other factors. If the AP is not managed by the AWC Plug-in, does not affect the floor map.
Wireless AP Icon | AP icons placed on the map is shown. The current status is displayed under the icon of the AP under the AWC Plug-in management. Radio signals being output in the selected radio band: In the format "[current channel]ch, [radio strength]%". (For example, "7ch, 100%") When Wireless Concierge AP Thinning is enabled and the AP in question is subject to thinning: Shown as "Standby". The AP in question is not providing radio output in the radio band being displayed. If the radio transmission is stopped by the Wireless AP Individual Configuration: Shown as "Stop". The AP in question is not providing radio output in the radio band being displayed. When you place your mouse cursor on an AP, the management information of the AP will pop up. Wireless AP Name MAC Address IP Address Used channels, bandwidth, and output strength of the currently displayed radio band. Number of Clients Last failed at (date and time last out of control)

Section 2

Shows the heatmap legend.
It shows the relationship between colors and signal strength or channels.
The legend can be made invisible or visible by using a checkbox in the floor map control section at the bottom of the page.

Section 3

Table 6: List of APs placed on the floor map
Item Name | Description
--- | ---
Details | Clicking this shows the device's model, MAC address, AP Profile, the number of associated clients for each radio, and tags, as well as the Device name, Management Status and IP address that are shown on the non-detailed view. Clicking Details again returns you to the default non-detailed view.
X AP | Shows the number of APs placed on the floor map.
Refresh Timer | Shows the status of the timer that automatically refreshes the page with the blue progress bar. The list is automatically refreshed at the interval configured on "Refresh Rates" > "Floor MAP (Wireless Status)" in the User Management menu. (The default is 1 minute.) You can also specify whether to pause or resume automatic updates by clicking Resume/Pause automatic update button on the right, or force the list to be updated by clicking the Manual update button.
Search Wireless AP | Entries in the list can be filtered by entering a partial string in the search box. The Search field lets you enter a partial string to match. The screen displays entries with that string in one of the following fields: "Device Name", "Management Status", "IP address", "MAC address" or "AP Profile" fields. To remove the filter, delete the string from the search field and press enter. Note The search is case-sensitive.
Filter by tag | Lets you filter APs with tags. Clicking tags uses the tags to filter the list. Clicking them again removes the filter. Clicking "Clear filter" removes the filter for all tags. Note To select tags, you have to switch the list to detailed mode (by clicking "View Details").
Tag | All tags are displayed under the "Search Wireless AP" box.
Status Icon | When the AP is managed by the AWC Plug-in, a green checkmark is displayed. When the AP is not managed by the AWC Plug-in, a red triangle is displayed.
Device Name | Shows the name given to the AP.
Management Status | Shows the Management Status of the AP.
IP Address | Shows the AP's IP address.

### Channel Mode

Section 1

Table 7: Floor Map
Item Name | Description
--- | ---
Floor Map (Background) | The map image specified when you created the map is shown. You can place icons for the APs in the righthand-side list. In addition, heat map is drawn with colors representing the reach and strength of the channel or signal. The drawing mode of the heat map can be selected from the floor map control. Note Even between wireless APs operating at the same radio strength, the size of output circle on the heat map may vary depending on the installation location and other factors. If the AP is not managed by the AWC Plug-in, does not affect the floor map.
Wireless AP Icon | AP icons placed on the map is shown. The current status is displayed under the icon of the AP under the AWC Plug-in management. Radio signals being output in the selected radio band: In the format "[current channel]ch, [radio strength]%". (For example, "7ch, 100%") When Wireless Concierge AP Thinning is enabled and the AP in question is subject to thinning: Shown as "Standby". The AP in question is not providing radio output in the radio band being displayed. If the radio transmission is stopped by the Wireless AP Individual Configuration: Shown as "Stop". The AP in question is not providing radio output in the radio band being displayed. When you place your mouse cursor on an AP, the management information of the AP will pop up. Wireless AP Name MAC Address IP Address Used channels, bandwidth, and output strength of the currently displayed radio band. Number of Clients Last failed at (date and time last out of control)

Section 2

Shows the heatmap legend.
It shows the relationship between colors and channels.
The legend can be made invisible or visible by using a checkbox in the floor map control section at the bottom of the page.

Section 3

Table 8: List of APs placed on the floor map
Item Name | Description
--- | ---
Details | Clicking this shows the device's model, MAC address, AP Profile, the number of associated clients for each radio, and tags, as well as the Device name, Management Status and IP address that are shown on the non-detailed view. Clicking Details again returns you to the default non-detailed view.
X AP | Shows the number of APs placed on the floor map.
Refresh Timer | Shows the status of the timer that automatically refreshes the page with the blue progress bar. The list is automatically refreshed at the interval configured on "Refresh Rates" > "Floor MAP (Wireless Status)" in the User Management menu. (The default is 1 minute.) You can also specify whether to pause or resume automatic updates by clicking Resume/Pause automatic update button on the right, or force the list to be updated by clicking the Manual update button.
Search Wireless AP | Entries in the list can be filtered by entering a partial string in the search box. The Search field lets you enter a partial string to match. The screen displays entries with that string in one of the following fields: "Device Name", "Management Status", "IP address", "MAC address" or "AP Profile" fields. To remove the filter, delete the string from the search field and press enter. Note The search is case-sensitive.
Filter by tag | Lets you filter APs with tags. Clicking tags uses the tags to filter the list. Clicking them again removes the filter. Clicking "Clear filter" removes the filter for all tags. Note To select tags, you have to switch the list to detailed mode (by clicking "View Details").
Tag | All tags are displayed under the "Search Wireless AP" box.
Status Icon | When the AP is managed by the AWC Plug-in, a green checkmark is displayed. When the AP is not managed by the AWC Plug-in, a red triangle is displayed.
Device Name | Shows the name given to the AP.
Management Status | Shows the Management Status of the AP.
IP Address | Shows the AP's IP address.

## Arranged AP List (Detail)

Clicking "Details" at the top of the list of placed APs on the "Floor Map Details" page extends the list to show additional information such as Device Type and AP Profile.
Information displayed on the list can be switched between "System info", "Radio info" and "Client info". By default, each AP's system information is displayed.

Section 1

Table 9
Item Name | Description
--- | ---
Details | Clicking "Details" again on the extended list shrinks the list to its default size.
X AP | Shows the number of wireless APs placed on the floor map.
Refresh Timer | Shows the status of the timer that automatically refreshes the page with the blue progress bar. The list is automatically refreshed at the interval configured on "Refresh Rates" > "Floor MAP (Wireless Status)" in the User Management menu. (The default is 1 minute.) You can also specify whether to pause or resume automatic updates by clicking Resume/Pause automatic update button on the right, or force the list to be updated by clicking the Manual update button.
Search Wireless AP | The Search field lets you enter a partial string to match. The screen displays entries with that string in one of the following fields: "Device Name", "Management Status", "IP address", "MAC address" or "AP Profile" fields. To remove the filter, delete the string from the search field and press enter. Note The search is case-sensitive.
"System Information" button | Switches the list content to system information for the APs placed on the floor map.
"Wireless Information" button | Switches the list content to the wireless configuration of the APs placed on the floor map.
"Client Info" button | Switches the list content to the number of clients (per radio) connected to each AP placed on the floor map.
Filter by tag | Lets you filter APs with tags. Clicking tags uses the tags to filter the list. Clicking them again removes the filter. Clicking "Clear filter" removes the filter for all tags.
Tag | All tags are displayed under the "Search Wireless AP" box.
"Tag" button | Lets you edit tags for the selected APs. To add the same tags to the APs and the floor map, check "Add the same tags to the floor map". Note If you paste a tag string from the clipboard, not all text may be visible. In that case, press Enter to make a tag from the entire pasted string. Note Pasting a tag containing a newline is not supported. Note Tag names may be truncated in the tag filter list on the Devices Map, Floor Map Details and Device Search pages. To avoid this, use shorter names for the tags. Enter a tag of your choice and press the Enter key. A single tag should be no more than 100 characters in length, with alphabets, numbers and symbols (including spaces). To delete a tag, click "x" to the right of the tag.

Section 2

Table 10: List of APs placed on the Floor Map (Detail)
Item Name | Description
--- | ---
System Info
Checkbox | To edit tags for APs, use the checkboxes to select APs and then click the "Edit Tags" button.
Device Name | Shows the name given to the AP.
Status | Shows the Management Status of the AP.
IP Address | Shows the AP's IP address.
Model | Shows the model name of the AP.
Version | Shows the firmware version applied to the AP.
MAC Address | Shows the device's MAC address.
AP Profile | Shows the AP Profile assigned to the AP.
Tag | Shows the tags set on the AP.
Radio info
Device Name | Shows the name given to the AP.
Radio 1 / Radio 2 / Radio 3 | Shows the frequency used on each radio band of the AP.
Channel | Shows the channel used on each radio band of the AP.
Tx Power | Shows the transmit power for each radio band of the AP.
Client info
Device Name | Shows the name given to the AP.
Radio 1 / Radio 2 / Radio 3 | Shows the frequency used on each radio band of the AP.
Associated Clients | Shows the number of clients (per radio band) connected to the AP.

10 Nov 2025 11:49