User Guide: AWC plug-in version 3.15.0 for VST-VRT

# IDS/IPS Settings

On this screen, you can configure IDS/IPS (Intrusion Detection/Protection System). These settings determine whether Rogue APs and Clients are detected, whether to execute a De-Auth attack, and whether to send a Rogue AP detection message to the Notification section.
Refer to Supported Functions per AP Model > Wireless Configuration" > "IDS/IPS Settings for APs that support this function.
IDS/IPS settings can be configured for each management group.

Section 1

Table 1
Item Name | Description
--- | ---
X Group | Shows the number of Management Groups.
Search Management Group | Lets you filter the list of Management Groups. The Search field lets you enter a partial string to match. The screen displays entries with that string in one of the following fields: "Management Group Name" or "Creation Date/Time". To remove the filter, delete the string from the search field and press enter. Note The search is case-sensitive.

Section 2

Table 2: IDS/IPS settings per management group
Item Name | Description
--- | ---
Management Group | Shows the Management Group name.
Rogue AP Detection | Shows whether to detect rogue APs.
Rogue Client Detection | Shows whether to detect rogue clients.
AP De-Auth Attack | Shows whether to attack rogue APs.
Edit (pencil icon) | Lets you edit the IDS/IPS configuration. Refer to Operation Reference > Miscellaneous Settings > Configure IDS/IPS Settings for more details.

Section 4

Table 3
Item Name | Description
--- | ---
Items per page | Specifies the number of items per page.
<< | Goes to the first page of the list.
(Page Number) | Shows the current page number in the list.
>> | Goes to the last page of the list.

10 Nov 2025 11:49