User Guide: AWC plug-in version 3.5.0 for VST-VRT

# Overview

Configure External IP Address for AWC Plug-in

In this section, we will show you the basic steps to configure a multi-channel (non-blanket) wireless network, through a quick tour. The steps include adding APs to the management database, putting APs on floor maps and scheduling AWC (Autonomous Wave Control) operation.
For simplicity, we assume that we are going to create the following network:

Table 1: Devices in the target network
Device Name | Node Name | Description
--- | --- | ---
AMF Master | AT-VAA | Running AMF Cloud
AlliedWare Plus Layer 3 Switch |  | IP Address: 192.168.1.1 Configured as a DHCP/NTP server
PoE+ AlliedWare Plus Switch |  | Supplying power with PoE+ On its ports for connecting wireless APs, VLAN 1 is the native VLAN and VLAN 100 is the only tagged VLAN that is allowed.
TQ4600 | TQ4600-6F-1 | IP Address: 192.168.1.100 MAC Address: 00:00:5E:00:53:00 Not joining the AMF network
TQ4600 | TQ4600-6F-2 | IP Address: 192.168.1.200 (statically assigned by DHCP server) MAC Address: 00:00:5E:00:53:20 Already joined the AMF network as a guest node
TQ4600 | TQ4600-6F-3 | IP Address: 192.168.1.201 (statically assigned by DHCP server) MAC Address: 00:00:5E:00:53:40 Already joined the AMF network as a guest node
Wireless Controller application container |  | AWC Plug-in

We assume that the following configuration items have been completed:

- The AMF network has been added to the management database of Vista Manager EX.
- The PoE+ switch has been properly configured to accommodate APs as guest nodes.
- The L3 switch has been configured with two VLANs, vlan1 (192.168.1.0/24) as the native VLAN and vlan100 (192.168.100.0/24) as the VLAN for wireless clients. DHCP pool for each VLAN was also setup.
- The PoE+ switch ports for wireless APs (and other required ports) have been configured with vlan1 as the native VLAN and vlan100 as the tagged VLAN for normal traffic.
- The APs have been configured separately with their IP addresses.

We also assume that we prepared the following image for the floor map.

## Configure External IP Address for AWC Plug-in

When using the AWC Plug-in to manage Wireless APs, it is necessary to register the IP address of the Wireless Controller application (AWC Plug-in) on the VST-VRT as an external IP address in the System Setting screen of the AWC Plug-in in advance.
If you have already configured the external IP address of the AWC plug-in correctly, this step is not necessary.

1. Click on System Setting from the AWC Plug-in menu.
   The "System Setting" screen appears.
2. In "External IP Address for AWC plug-in" under "IP Address Settings", select the IP address of the Wireless Controller application (i.e., AWC Plug-in) on the VST-VRT from the dropdown list.
3. Click on "Save" button in the right side of "IP Address Settings".

22 Apr 2021 15:29