User Guide: AWC plug-in version 3.9.0 for VST-VRT

# Recommended Settings for TQ5000/6000 Series

When designing a cell-based (non-blanket) or AWC-CB wireless LAN using TQ5403/5403e/6602 and TQm5403, the following settings are recommended to ensure a stable wireless network.
Default settings are recommended for setting items not listed in this table. These are only recommended values, and you may need to adjust the settings depending on your environment.

Table 1: Recommended Settings for TQ5000/6000 Series
Item Name | Options included in | Scope of setting | Cell-based | AWC-CB | Comment
--- | --- | --- | --- | --- | ---
TQ5403 TQm5043 TQ5403e | TQ6602 | TQ5403 TQ5403e | TQ6602
Management Group | Management Group | - | Registered APs per management group: 50 or less |
Neighbor Managed AP Detection | AWC Settings | Whole AP | Disable when AWC Auto calc is not used | Disable when AWC Auto calc is not used |
Airtime Fairness | AP Profile | Per Band | Disable (default) | Disable (required, default) |
Legacy Rate Sets | AP Profile | Per Band | Disable 1, 2Mbps for 2.4GHz | Disable 1, 2Mbps for 2.4GHz |
RTS Threshold | AP Profile | Per Band | 2347 (default) | 2347 (required, default) |
Band Steering | AP Profile | Whole AP | Disable (default) | Disable (required, default) |
NoAck | - | Per Band | Disable (default) | Enable (default) | Disable (default) | Enable (default) | If an AP that has been used as a standalone is added to the management, check the settings on the Web GUI of the AP itself (Settings > QoS) and change them to the defaults shown on the left.
APSD | AP Profile | Per Band | Disable (default) | Enable (default) | Disable (default) | Enable (default) |
Neighbor AP Detection | AP Profile | Per Band | Disable when Neighbor AP Detection is disabled and AWC Auto Calc is set to low precision or is disabled | Disable (required) |
MU-MIMO | AP Profile | Per Band | - | Disable (default) | - | Not Supported, Disable (required, default) |
OFDMA | AP Profile | Per Band | - | Disable (default) | - | Not Supported, Disable (required, default) |
Management Frame Protection | AP Profile/ CB Profile | Per VAP | Disable | Disable |
Broadcast Key Refresh Rate | AP Profile/ CB Profile | Per VAP | 0 (default) | Not Supported, 0 (required, default) |
RADIUS Accounting | AP Profile/ CB Profile | Per VAP | Disable (default) | Not Supported, Disable (required, default) |
Dynamic VLAN | AP Profile/ CB Profile | Per VAP | Disable | Not Supported, Disable (required) | Standalone AP: Disabled by default AP Profile: Enabled by default CB Profile: Always disabled
Fast Roaming | AP Profile/ CB Profile | Per VAP | Disable (default) | Not Supported, Disable (required, default) |
Inactivity Timer | AP Profile/ CB Profile | Per VAP | 300 (default) | Not Supported, 300 (required, default) |
Duplicate AUTH received | AP Profile/ CB Profile | Per VAP | Ignore | - | Ignore | - |
Association Advertisement | AP Profile/ CB Profile | Per VAP (in the case of AWC-CB, all CB VAPs in the relevant radio band.) | Enable | Enable (required) |
DTIM Period | AP Profile/ CB Profile | Per VAP | Normal: 1 (default) | Normal: 1 (default) When expecting to reduce device battery consumption: 3 |
Proxy ARP | AP Profile/ CB Profile | Per VAP (in the case of AWC-CB, all CB VAPs in the relevant radio band.) | Disable for data communication Enable for IP telephony system | Enable (required) |
RSSI Threshold | CB Profile | All CB-VAPs | - | 30 |

21 Oct 2022 11:59