# AWC Plug-in User Guide 3.1.0

# Reboot AP and Update AP Firmware

Reboot AP
Update AP Firmware
Firmware Registration
Edit Firmware
Delete Firmware
Assign Firmware To AP
Cancel Assigned Firmware
Update Firmware

This section explains how to reboot and update managed APs.

> Note

> > When communication between the AWC Plug-in and an AP is lost after starting a reboot or an update, the AWC Plug-in shows the AP status as "Failed" if it cannot restore communication after ten minutes.

## Reboot AP

> Note

> > The maximum number of APs you can reboot in a single operation is 350.

1. Select "Wireless Configuration" > "AP Settings" from the AWC Plug-in menu.
2. From the list of APs, check the checkboxes of the APs to reboot.
3. Put the mouse cursor on the spanner icon at the top right of the screen and select "Reboot" from the submenu.
4. The "Reboot" dialog box will appear.

   Table 1: Confirmation dialog box
   Item Name | Description
   --- | ---
   "OK" button | Reboots the selected APs.
   "Cancel" button | Cancels the reboot operation.

5. Click "OK".
6. The reboot process begins. The message "Reboot completed" will appear when it is finished. Click the "Close" button.

## Update AP Firmware

You can update the firmware of managed AP's from the AWC Plug-in's management web interface.
The steps to update the firmware are:

- Upload firmware files to the AWC Plug-in
- Assign a firmware file to each managed AP
- Apply the assigned firmware file to APs

Even if several different AP models are used on your network, you can update the firmware of those APs in a single operation by uploading and assigning appropriate firmware for each AP.
Please note that this function only supports update from the following firmware versions:

- TQ Series:
  TQ2450, TQ3200, TQ3400, TQ3600, TQ4400, TQ4400e, TQ4600
  Firmware Version 4.1.x Bxx (4.1.1 B05 or later) and 4.2.x Bxx
  TQ5403
  Firmware Version 5.0.x, 5.1.x and 5.2.x
  TQm5403, TQ5403e
  Firmware Version 5.1.x and 5.2.x
- MWS AP Series
  MWS600AP
  Firmware Version 2.2.4
  MWS1750AP
  Firmware Version 2.2.4 or later
  MWS2533AP
  Firmware Version 2.2.3
- SDN/OpenFlow-capable TQ Series
  TQ4400, TQ4600
  Firmware Version 4.1.x Sxx
  AT-TQ5403, AT-TQ5403e
  Firmware Version 5.2.x

If you are managing APs with older firmware versions, update them to the supported versions described above using the "AT-TQ Series Firmware Update" tool, or with the AP's management web interface. Please refer to the Installation Guide's "AT-TQ Firmware Update Utility / Usage" section for more details on the tool.

### Firmware Registration

First, you have to upload firmware files to the AWC Plug-in.

1. Select "Wireless Maintenance" > "Firmware Registration" from the AWC Plug-in menu.
   The "Wireless Maintenance/Add Firmware" page will appear.
2. Click "Register" at the top right of the Content section.
3. The "Firmware Registration" dialog box will appear.

   Table 2: "Firmware Registration" dialog box.
   Item Name | Description
   --- | ---
   Firmware File | A firmware file to upload to the AWC Plug-in. Specify it by clicking "Select File" and selecting a file on the standard file selection dialog box. You can only select a single firmware file at a time. Repeat the steps in this section to upload multiple firmware files.
   Management Group | Select the Management Groups whose member APs can use the firmware file. You cannot uncheck "Default Wireless Group". Search Wireless Management Group: Groups in the list can be filtered by entering a partial name in the search box. The Search field lets you enter a partial string to match. The screen displays entries with that string in their name. To remove the filter, delete the string from the Search field and press Enter. Note The search is case-sensitive.
   Series | Select an AP series for which the firmware file is built. TQ Series MWS-AP Series TQ Series - SDN/OpenFlow
   Model | Select an AP model type for which the firmware file is built. Options here vary depending on the selected "Series". When the "Series" is either "TQ Series" or "TQ Series - SDN/OpenFlow" Auto Detect: the plug-in determines the AP model for which the uploaded firmware is built. When the "Series" is "MWS-AP Series" Auto Detect option is not available. Select a model from the following list. MWS600AP MWS1750AP MWS2533AP
   Version | Specify a version of the firmware file to upload. Auto detection is possible for TQ series' firmware file. When the "Series" is either "TQ Series" or "TQ Series - SDN/OpenFlow" Auto Detect: the plug-in determines the firmware version from the uploaded firmware file. When the "Series" is "MWS-AP Series" Manually enter a version in "x.x.x.Bxx" format. Auto Detect option is not available.
   "Add" button | Upload the firmware file. It shows an error message if the selected file is invalid or too large for a firmware file.
   "Cancel" button | Cancels the firmware upload.

4. Select a firmware file to upload.
5. Select the Management Groups whose member APs can use the firmware file and a series for which the firmware file is built.

   Also specify a model and a version if you select "MWS-AP Series".
6. Click "Add". Now you can see the uploaded firmware is listed on the "Add Firmware" page.

#### Edit Firmware

You can change Management Groups for the uploaded firmware.

> Note

> > You cannot change the Series, Device Type or Version for the uploaded firmware. If you want to change those parameters, you have to upload the same firmware file with the new parameter values.

1. Click "Edit" (the pencil icon) to the right of the firmware file you want to change, on the "Wireless Maintenance / Add Firmware" page.

2. The "Firmware Edit" dialog box will appear.

   Table 3: "Firmware Edit" dialog box.
   Item Name | Description
   --- | ---
   Firmware File | Shows the firmware filename which has been uploaded to the AWC Plug-in.
   Management Group | Select the Management Groups whose member APs can use the firmware file. You cannot uncheck "Default Wireless Group". Search Wireless Management Group: Groups in the list can be filtered by entering a partial name in the search box. The Search field lets you enter a partial string to match. The screen displays entries with that string in their name. To remove the filter, delete the string from the Search field and press Enter. Note The search is case-sensitive.
   Series | Shows the series of APs for which the firmware file is built.
   Model | Shows the models of APs for which the firmware file is built.
   Version | Shows the version of the firmware file.
   "Save" button | Save the change to the Management Groups.
   "Cancel" button | Discard the change to the Management Groups.

3. Select the Management Groups whose member APs can use the firmware file.

   > Note

   > > You cannot uncheck "Default Wireless Group".

4. Click "Save". You can see the change on the "Wireless Maintenance / Add Firmware" page.

#### Delete Firmware

You can delete uploaded firmware files that were added by mistake or are no longer needed.

1. Click the "Delete" (trashbin icon) button for the firmware file to be deleted, on the "Wireless Maintenance / Add Firmware" page.

2. The "Confirm" dialog box will appear.
   Click "Delete" to delete the firmware file.
   To cancel the deletion, click "Cancel".

### Assign Firmware To AP

Once a firmware file has been uploaded, you can assign it to managed APs for future updates.

1. Click the "Assign" button for the firmware file on the "Wireless Maintenance / Add Firmware" page.
2. The "Firmware Assignment" dialog box will appear.
   The dialog box title shows the firmware file's target model and version, in the format "[Device Type: AT-TQxxxx, Version: x.x.x.Bxx]".

3. Select the managed APs that you want to assign the firmware file.
   In case there are a lot of managed APs, you can filter the APs to display by using the Search Form.
   The Search field lets you enter a partial string to match. The screen displays entries with that string in one of the following fields: "Device Name", "Current Firmware", "IP address", "MAC address", "Management Group", "Floor Map Name", "AP Profile", "Device Type" or "Serial Number". To remove the filter, delete the string from the Search field and press Enter.

   > Note

   > > The search is case-sensitive.

4. Click "Save".
   The firmware file has been assigned to the selected managed APs.
   From now on, the firmware file will be applied to the APs when you manually apply firmware, or the plug-in's scheduled task applies assigned firmware automatically.
   The firmware file assigned to an AP can be reviewed in the Wireless AP Details or Wireless AP Status Details pages' Basic Information section.

#### Cancel Assigned Firmware

1. Click the "Assign" button for the firmware file on the "Wireless Maintenance / Add Firmware" page.
2. The "Firmware Assignment" dialog box will appear.
   The dialog box title shows the firmware file's target model and version, in the format "[Device Type: AT-TQxxxx, Version: x.x.x.Bxx]".

3. Click the "Remove" button at the top right of the dialog box.
   APs to which the selected firmware file is currently assigned are listed.
4. Select the managed APs from which you want to remove the assigned firmware file.
5. Once you have finished the selection, click "Save".
   The assigned firmware file for the selected APs has been cleared.

### Update Firmware

> Note

> > The number of APs that can be updated at a time depends on the traffic rate between the AWC Plug-in and each AP.
> > If the traffic rate between the AWC Plug-in and each AP is 1 Gbps, the maximum number of APs that can be updated at one time is approximately 200 for the TQ5403, TQ5403e and TQm5403, otherwise it is up to 350 units.
> > If the bands are used for other communication, the maximum may be less than the above number.

> Note

> > If you perform update operations in succession, put a wait (30 sec per 1 AP) between operations.

> Note

> > You can create a scheduled task to update firmware.
> > Refer to Manage Task Scheduling for more details on Scheduling.

1. Select "Wireless Configuration" > "AP Settings" from the AWC Plug-in menu.
2. Select the APs whose firmware you want to update.
3. Put the mouse cursor on the spanner icon at the top right of the screen and select "Update Firmware" from the submenu.
4. The "Upgrade Firmware" dialog box will appear.

   Table 4: "Upgrade Firmware" dialog box.
   Item Name | Description
   --- | ---
   Device Name | Shows the device name of an AP.
   IP Address | Shows the IP Address of a managed AP.
   MAC Address | Shows the MAC Address of a managed AP.
   Management Status | Shows the Management Status of an AP.
   Current Firmware | Always shows "-".
   Assigned Firmware | Shows the target device type and version of a firmware file that has been assigned to the AP.
   "OK" button | Updates the firmware for the AP.
   "Cancel" button | Closes the dialog box without updating firmware files.

5. Specify a firmware file.
6. Click "OK".
7. The update process begins. The message "Firmware upgrade completed" will appear when it finished. Click the "Close" button.

13 Mar 2020 16:32