# AWC Plug-in User Guide 3.1.0

# Floor Map

Floor Map List
Panel View
List View
Floor Map [Wireless Status View]
Arranged AP List (Detail)
Floor Map [Associated Client View]
Client Location Estimation View
Client Association View
Associated Client List (Detail)
Client Definition List
Associated Client History View
Associated Client Location Estimation History
Associated Client Roaming History
Associated Client History (Detail)
Floor Map [Smart Connect View]
Smart Connect AP List (Detail)
Floor Map [Rogue AP View]
Rogue AP List (Detail)
Floor Map [Add AP to Map]
Floor Map [Edit Area]

This page allows you to create floor maps to manage APs more efficiently.
Clicking a floor map panel shows its details.

> Note

> > The page is periodically refreshed to display the latest information.

> Note

> > Please do not use the automatic scroll feature of your mouse wheel on the page.

> Note

> > Long floor map names may be truncated on the "Floor Map List" in the panel or list view and the "Floor Map Details" page.
> > To see an entire name, go to the "Floor Map List" > "List View" icon > "Pencil" icon > "Edit Floor Map" page.

> Note

> > If you sort by IP address, the addresses in an AP list are sorted in lexicographical order.

## Floor Map List

### Panel View

Section 1

Table 1: Floor Map List's command buttons
Item Name | Description
--- | ---
"Switch View" button | Switch the floor map list between "Panel View" and "List View".
"Tag" button | Note The "Edit Tags" button cannot be used in Panel View. Edit tags in List View.
"Create" button | Opens the "Create Floor Map" dialog box. Refer to Operation Reference > Floor Map > Configure Floor Maps for more details.

Section 2

Table 2: Floor Map List
Item Name | Description
--- | ---
X Deployment Map | Shows the number of floor maps.
Search Floor Map | Entries in the list can be filtered by entering a partial string in the search box. The Search field lets you enter a partial string to match. The screen displays entries with that string in one of the following fields: "Floor Map Name", "Management Group Name" or "Tag". To remove the filter, delete the string from the Search field and press Enter. Note The search is case-sensitive.
Floor Map Panels | Each floor map is shown as a panel. The name of the floor map and the number of APs placed on the map are shown below the panel. When an Admin user hovers over a panel, that panel will become half-opaque, and "Edit" (pencil) and "Delete" (trashbin) buttons will appear at the top right of the panel Clicking the panel opens the "Floor Map Details" page for the floor map. When a floor map panel is shown in red, one or more APs on the floor map has an issue. "Edit" (pencil) button: Opens the "Edit Floor Map" dialog box to edit its name, image file, tags and notes. "Delete" (trashbin) button: Opens the "Delete Floor Map" dialog box to let you delete the floor map. "View Details >>": Moves to the "Floor Map Details" page. Comment Balloon (On mouse-over): Shows the notes for the floor map, if any.

### List View

Clicking the "Switch View" button in the Panel View changes the screen to List View.

Section 1

Table 3
Item Name | Description
--- | ---
"Panel View" button | Switches from List View to Panel View.
"Tag" button | Lets you edit tags for the selected floor maps. Note If you paste a tag string from the clipboard, not all text may be visible. In that case, press Enter to make a tag from the entire pasted string. Note Pasting a tag containing a newline is not supported. Note Tag names may be truncated in the tag filter list on the Nodes Map, Floor Map Details and Device Search pages. To avoid this, use shorter names for the tags. Enter a tag of your choice and press the Enter key. A tag can contain up to 100 characters, but cannot contain successive spaces. To delete a tag, click "x" to the right of the tag.
"Create" button | Opens the "Create Floor Map" dialog box. Refer to Operation Reference > Floor Map > Configure Floor Maps for more details.

Section 2

Table 4: Floor Map List
Item Name | Description
--- | ---
X Deployment Map | Shows the number of floor maps.
Search Floor Map | Entries in the list can be filtered by entering a partial string in the search box. The Search field lets you enter a partial string to match. The screen displays entries with that string in one of the following fields: "Floor Map Name", "Management Group Name" or "Tag". To remove the filter, delete the string from the Search field and press Enter. Note The search is case-sensitive.
Checkbox | To edit tags for floor maps, use the checkbox to select the maps and click this button.
Status Icon | Overall status of the APs on the floor map is indicated by an icon. A green checkmark means everything is normal. A red triangle indicates some APs on the map have an issue.
Floor Map Name | Shows the name of the floor map.
Management Group | Shows Management Groups for the floor map.
Deployed APs | Shows the number of wireless APs placed on the floor map.
Tag | Shows tags added to the floor map.
"Edit" (pencil) button: | Lets you edit the floor map.
"Delete" (trashbin) button: | Lets you delete the floor map.
Comment Balloon (On mouse-over) | Shows the notes for the floor map, if any.

Section 3

Table 5
Item Name | Description
--- | ---
Items per page | Specifies the number of items per page.
<< | Go to the first page in the list.
(Page Number) | Shows the current page number in the list.
>> | Go to the last page in the list.

## Floor Map [Wireless Status View]

Clicking on a floor map panel shows the "Floor Map Details" page.
The floor map is displayed in the center of the Content section and a list of APs is shown on the right side of the Content section.

> Note

> > The status displayed for an unreachable AP is the status that was last collected.

> Note

> > If you try to move an AP icon, it may move to an unintended position and your mouse cursor and the icon may become out of sync.
> > If this occurs, release your mouse button and drag the icon again.

> Note

> > If you try to place an AP on a floor map that was deleted by another user, you will be brought back to the "Floor Map Details" page without any error message. In such cases, please check if the floor map still exists on the "Floor Map List" page.

Section 1

Table 6: Floor Map
Item Name | Description
--- | ---
Floor Map Name | Shows the floor map name.
Radio dropdown menu | Lets you select a radio band to show on the map, from Radio 1, 2 or 3.
View Selection dropdown menu | Lets you change what information is displayed on the Floor Map Details screen. Wireless Status View Associated Client View Smart Connect View Rogue AP View Add AP to Map Edit Area
Floor Map (Background) | The map image specified when you created the map is shown. You can place icons for the APs in the righthand-side list.
Wireless AP Icon | AP icons placed on the map is shown. Below each icon, the channel and transmit power for the AP are displayed. Notes on icons: When an AP is managed by the AWC Plug-in, its channel and transmit power is shown below its icon. The size and the color of a circle around its icon represent its channel and signal strength. If the AP is not managed by the AWC Plug-in, nothing additional is displayed for its icon. Note Even when an AP is managed by the AWC Plug-in, nothing is displayed if its radio is disabled.

Section 2

Table 7: List of APs placed on the floor map
Item Name | Description
--- | ---
Details | Clicking this shows the device's model, MAC address, AP Profile, the number of associated clients for each radio, and tags, as well as the Device name, Management Status and IP address that are shown on the non-detailed view. Clicking Details again returns you to the default non-detailed view.
X AP | Shows the number of APs placed on the floor map.
Refresh Timer | Shows the status of the timer that automatically refreshes the page. The blue portion of the bar shows the elapsed time since the last refresh and the grey or white portion shows the time to the next refresh. The list is automatically refreshed at the interval configured on "Refresh Rates" > "Floor MAP (Wireless Status)" in the User Management menu. (The default is 1 minute.)
Search Wireless AP | Entries in the list can be filtered by entering a partial string in the search box. The Search field lets you enter a partial string to match. The screen displays entries with that string in one of the following fields: "Device Name", "Management Status", "IP address", "MAC address" or "AP Profile" fields. To remove the filter, delete the string from the Search field and press Enter. Note The search is case-sensitive.
Filter by tag | Lets you filter APs with tags. Clicking tags uses the tags to filter the list. Clicking them again removes the filter. Clicking "Clear filter" removes the filter for all tags. Note To select tags, you have to switch the list to the detailed mode (by clicking "View Details").
Tag | All tags are displayed under the "Search Wireless AP" box.
Status Icon | When the AP is managed by the AWC Plug-in, a green checkmark is displayed. When the AP is not managed by the AWC Plug-in, a red triangle is displayed.
Device Name | Shows the name given to the AP.
Management Status | Shows the Management Status of the AP.
IP Address | Shows the AP's IP address.

Section 3

Shows the heatmap legend.
This shows the relationship between colors and signal strength or channels.
The legend can be made invisible or visible by using a checkbox in the floor map control section at the bottom of the page.
Color conventions depend on the floor map drawing mode.

- Power

- Channel

Section 4

In Wireless Status View, the "Healthiness Icon" is disabled.

Table 8: Floor Map Control
Item Name | Description
--- | ---
Drawing Mode | Lets you select what to show on the heatmap. Options are power (signal strength) and channel.
Grid | Lets you enable or disable grid lines on the floor map. Checking this shows grid lines on the floor map.
Legend | Lets you enable or disable the legend. Check to display.
Details | Whether to display the list of placed APs. Check to display.
Floor Area | If areas have been created on the floor map (using the Edit Area page), whether to display the areas. Check to display.
Power Limit | Specify the minimum signal strength to show in colors on the heatmap.
Opacity | Specify the opacity of the floor map background image.

### Arranged AP List (Detail)

Clicking "Details" at the top of the list of placed APs on the "Floor Map Details" page extends the list to show additional information such as Device Type and AP Profile.
Information displayed on the list can be switched between "System info", "Radio info" and "Client info". By default, each AP's system information is displayed.

Section 1

Table 9
Item Name | Description
--- | ---
Details | Clicking "Details" again on the extended list shrinks the list to its default size.
X AP | Shows the number of wireless APs placed on the floor map.
Refresh Timer | Shows the status of the timer that automatically refreshes the page. The blue portion of the bar shows the elapsed time since the last refresh and the grey or white portion shows the time to the next refresh. The list is automatically refreshed at the interval configured on "Refresh Rates" > "Floor MAP (Wireless Status)" in the User Management menu. (The default is 1 minute.)
Search Wireless AP | The Search field lets you enter a partial string to match. The screen displays entries with that string in one of the following fields: "Device Name", "Management Status", "IP address", "MAC address" or "AP Profile" fields. To remove the filter, delete the string from the Search field and press Enter. Note The search is case-sensitive.
"System Information" button | Switches the list content to system information for the APs placed on the floor map.
"Wireless Information" button | Switches the list content to the wireless configuration of the APs placed on the floor map.
"Client Info" button | Switches the list content to the number of clients (per radio) connected to each AP placed on the floor map.
Filter by tag | Lets you filter APs with tags. Clicking tags uses the tags to filter the list. Clicking them again removes the filter. Clicking "Clear filter" removes the filter for all tags.
Tag | All tags are displayed under the "Search Wireless AP" box.
"Tag" button | Lets you edit tags for the selected APs. To add the same tags to the APs and the floor map, check "Add the same tags to the floor map". Note If you paste a tag string from the clipboard, not all text may be visible. In that case, press Enter to make a tag from the entire pasted string. Note Pasting a tag containing a newline is not supported. Note Tag names may be truncated in the tag filter list on the Nodes Map, Floor Map Details and Device Search pages. To avoid this, use shorter names for the tags. Enter a tag of your choice and press the Enter key. A tag can contain up to 100 characters, but cannot contain successive spaces. To delete a tag, click "x" to the right of the tag.

Section 2

Table 10: List of APs placed on the Floor Map (Detail)
Item Name | Description
--- | ---
System info
Checkbox | To edit tags for APs, use the checkboxes to select APs and then click the "Edit Tags" button.
Device Name | Shows the name given to the AP.
Management Status | Shows the Management Status of the AP.
IP Address | Shows the AP's IP address.
Model | Shows the model name of the AP.
MAC Address | Shows the device's MAC address.
AP Profile | Shows the AP Profile assigned to the AP.
Tag | Shows the tags set on the AP.
Radio info
Device Name | Shows the name given to the AP.
Channel (Radio1) Channel (Radio2) Channel (Radio3) | Shows the channel used on each radio band of the AP.
Tx Power (Radio1) Tx Power (Radio2) Tx Power (Radio3) | Shows the transmit power for each radio band of the AP.
Client info
Device Name | Shows the name given to the AP.
Associated Clients (Radio1) Associated Clients (Radio2) Associated Clients (Radio3) | Shows the number of clients (per radio band) connected to the AP.

## Floor Map [Associated Client View]

If you select "Associated Client View" from the dropdown menu on Floor Map Details, the screen switches to the Associated Client View screen.
If AWC was able to estimate the location of the associated clients, then this view shows the clients' estimated locations on the Floor Map. This is called the Associated Client Location Estimation display. If AWC was not able to estimate the location of the associated clients, then this view shows the clients arranged near their associated AP, to show affiliation. This is called the Client Association View display. These display optiions may be mixed, so that the Associated Client View screen shows a mix of location estimation and affiliation display for connected clients.

### Client Location Estimation View

> Note

> > The Client Location Estimation View will be supported in an upcoming release.

The position estimated from the radio wave of the associated client detected by the AP is reflected in the coordinates on the Floor Map and displayed.
This can occur when all of the following conditions are met:

- The wireless client has connected to a Blanket VAP.
- The system setting "Associated Client Location Estimation History" is enabled.
- Location information is calculated by the Associated Client Location Estimation function.

If any of these conditions are not met, Client Association View will be displayed instead.

> Note

> > When using the Client Location Estimation View, set the floor map dimensions (vertical / horizontal) correctly and match AP placement with the actual environment.

> Note

> > System clocks on all the managed APs and the server running the AWC Plug-in must be synchronized.

Section 1

Table 11: Floor Map
Item Name | Description
--- | ---
Floor Map Name | Shows the floor map name.
"Client Definition" button | Shows the Client Definition List dialog box.
Radio dropdown menu | Select which radio band information to display from Radio 1, Radio 2, Radio 3, or "All Radios". The default is "All Radios". If you select "All Radios", Associated Client Information for all bands (Radio 1, Radio 2, and Radio 3) will be displayed.
View Selection dropdown menu | Lets you change what information is displayed on the Floor Map Details screen. Wireless Status View Associated Client View Smart Connect View Rogue AP View Add AP to Map Edit Area
Floor Map (Background) | The map image specified when you created the map is shown.
Wireless AP Icon | The AP icon placed on the floor map is displayed. Below the icon, the number of associated clients is displayed. When you click an AP icon, only clients connected to the AP are displayed in the associated client list.
Wireless Client icon | Shows the wireless clients that have been connected to the AP on the map. The Estimation Location of a wireless client is indicated by the Associated Client icon (a laptop shape). The color of the circle surrounding the Associated Client icon represents the reliability of the location estimation (see the legend). You can click the Associated Client icon to see the probable circle of location based on the estimation reliability. You can also hover over the Associated Client icon to see popup information about the estimated client.

Section 2

Table 12: Floor Map Associated Client List
Item Name | Description
--- | ---
Details | You can click here to see client details such as Hostname, Username (based on WPA Enterprise), Duration, Client Name, Notes, SSID, Associating AP, and RSSI, in addition to the items displayed by default (MAC and IP addresses). Clicking Details again returns you to the default non-detailed view.
X Client | Shows the number of clients connected to the AP that is selected on the floor map.
Refresh Timer | Shows the status of the timer that automatically refreshes the page. The blue portion of the bar shows the elapsed time since the last refresh and the grey or white portion shows the time to the next refresh. The list is automatically refreshed at the interval configured on "Refresh Rates" > "Floor MAP (Associated Client)" in the User Management menu. (The default is 5 seconds.)
Search Associated Clients | Entries in the list can be filtered by entering a partial string in the search box. The Search field lets you enter a partial string to match. The screen displays entries with that string in one of the following fields: "MAC Address", "IP Address", "SSID" or "Associating AP". To remove the filter, delete the string from the Search field and press Enter. Note The search is case-sensitive.
"Show Client History" checkbox | Switches the page to Associated Client History.
Checkbox | Lets you select wireless clients to be shown on the floor map. When you select a client, an icon and the MAC address of the client are shown near the AP with which the client is associated.
MAC Address | Shows the MAC address of the wireless client.
IP Address | Shows the IP address of the wireless client.

Section 3

Shows the legend for the Associated Client View.
The color of each cell in the legend represents the reliability of the location estimation of clients shown on the map.
The legend can be made invisible or visible by using a checkbox in the floor map control section at the bottom of the page.

Section 4

In the Associated Client Location Estimation View, "Drawing Mode", "Healthiness Icon", and "Power Limit" are irrelevant and disabled.

Table 13: Floor Map Control
Item Name | Description
--- | ---
Grid | Lets you enable or disable grid lines on the floor map. Checking this shows grid lines on the floor map.
Legend | Lets you enable or disable the legend. Check to display.
Details | Whether to display the Associated Client List. Check to display. Check to display.
Floor Area | If areas have been created on the floor map (using the Edit Area page), whether to display the areas. Check to display.
Opacity | Specify the opacity of the floor map background image.

### Client Association View

This view uses a link line to show an association between a client and an AP.

Section 1

Table 14: Floor Map
Item Name | Description
--- | ---
Floor Map Name | Shows the floor map name.
"Client Definition" button | Shows the Client Definition List dialog box.
Radio dropdown menu | Select which radio band information to display from Radio 1, Radio 2, Radio 3, or "All Radios". The default is "All Radios". If you select "All Radios", Associated Client Information for all bands (Radio 1, Radio 2, and Radio 3) will be displayed.
View Selection dropdown menu | Lets you change what information is displayed on the Floor Map Details screen. Wireless Status View Associated Client View Smart Connect View Rogue AP View Add AP to Map Edit Area
Floor Map (Background) | The map image specified when you created the map is shown.
Wireless AP Icon | The AP icon placed on the floor map is displayed. Below the icon, the number of associated clients is displayed. When you click an AP icon, only clients connected to the AP are displayed in the associated client list.
Wireless Client icon | An icon representing an associated client. Clients checked on the list will be displayed on the floor map. The position the Client icon is displayed does not indicate the client's actual geographical location on the floor.

Section 2

Table 15: Floor Map Associated Client List
Item Name | Description
--- | ---
Details | You can click here to see client details such as Hostname, Username (based on WPA Enterprise), Duration, Client Name, Notes, SSID, Associating AP, and RSSI, in addition to the items displayed by default (MAC and IP addresses). Clicking Details again returns you to the default non-detailed view.
X Client | Shows the number of clients connected to the AP that is selected on the floor map.
Refresh Timer | Shows the status of the timer that automatically refreshes the page. The blue portion of the bar shows the elapsed time since the last refresh and the grey or white portion shows the time to the next refresh. The list is automatically refreshed at the interval configured on "Refresh Rates" > "Floor MAP (Associated Client)" in the User Management menu. (The default is 5 seconds.)
Search Associated Clients | Entries in the list can be filtered by entering a partial string in the search box. The Search field lets you enter a partial string to match. The screen displays entries with that string in one of the following fields: "MAC Address", "IP Address", "SSID" or "Associating AP". To remove the filter, delete the string from the Search field and press Enter. Note The search is case-sensitive.
"Show Client History" checkbox | Switches the page to Associated Client History.
Checkbox | Lets you select wireless clients to be shown on the floor map. When you select a client, an icon and the MAC address of the client are shown near the AP with which the client is associated.
MAC Address | Shows the MAC address of the wireless client.
IP Address | Shows the IP address of the wireless client.

Section 3

Shows the legend for the Associated Client View.
The color of each cell in the legend represents the reliability of the location estimation of clients shown on the map.
The legend can be made invisible or visible by using a checkbox in the floor map control section at the bottom of the page.

Section 4

In the Client Association View, "Drawing Mode", "Healthiness Icon", and "Power Limit" are irrelevant and disabled.

Table 16: Floor Map Control
Item Name | Description
--- | ---
Grid | Lets you enable or disable grid lines on the floor map. Checking this shows grid lines on the floor map.
Legend | Lets you enable or disable the legend. Check to display.
Details | Whether to display the Associated Client List. Check to display. Check to display.
Floor Area | If areas have been created on the floor map (using the Edit Area page), whether to display the areas. Check to display.
Opacity | Specify the opacity of the floor map background image.

### Associated Client List (Detail)

Clicking "Details" at the top of the client list in the "Associated Client View" extends the list to show additional information including system information, wireless information and statistics.

Table 17: Associated Client List (Detail)
Item Name | Description
--- | ---
Details | Clicking this shows extra data, including the SSID, Associated AP and connection Duration, in addition to the default items (IP and MAC addresses). Clicking Details again returns you to the default non-detailed view.
X Client | Shows the number of clients connected to the AP that is selected on the floor map.
Refresh Timer | Shows the status of the timer that automatically refreshes the page. The blue portion of the bar shows the elapsed time since the last refresh and the grey or white portion shows the time to the next refresh. The list is automatically refreshed at the interval configured on "Refresh Rates" > "Floor MAP (Associated Client)" in the User Management menu. (The default is 5 seconds.)
Search Associated Clients | Entries in the list can be filtered by entering a partial string in the search box. The Search field lets you enter a partial string to match. The screen displays entries with that string in one of the following fields: "MAC Address", "IP Address", "SSID" or "Associating AP". To remove the filter, delete the string from the Search field and press Enter. Note The search is case-sensitive.
"System Info" / "Wireless Info" / "Statistics" buttons | Switches the contents of the list.
System info
Checkbox | Lets you select wireless clients to be shown on the floor map. When you select a client, an icon and the MAC address of the client are shown near the AP with which the client is associated. A selection made through the detailed list view will remain when you go back to default (simpler) client list view.
MAC Address | Shows the MAC address of the wireless client.
IP Address | Shows the IP address of the wireless client.
Hostname (NetBIOS) | Shows the NetBIOS host name of the wireless client.
Username (WPA Enterprise) | Shows the RADIUS username when using WPA Enterprise.
Duration | Shows the time duration for which the client has been connected to the AP. (TQ series only.)
Client Name | Shows the Client Name if defined in the "Client Definition List" dialog box.
Notes | Shows any comments entered in the "Client Definition List" dialog box.
Radio info
MAC Address | Shows the MAC address of the wireless client.
SSID | Shows the SSID the client is associated with.
Associating AP | Shows the device name of the AP the client is associated with.
RSSI | Shows the RSSI (Received Signal Strength Indicator) of the wireless client.
Noise | Shows the strength of the noise that is interfering with the client communication.
SNR | Shows the Signal to Noise Ratio. A larger SNR means there is less noise influence.
Statistics
MAC Address | Shows the MAC address of the wireless client.
Tx Packets | Shows the number of the packets sent to the client.
Tx Bytes | Shows the total size of the packets sent to the client.
Tx Drop Packets | Shows the number of discarded packets to be sent to the client.
Tx Drop Bytes | Shows the number of discarded bytes to be sent to the client.
Rx Packets | Shows the number of the packets received from the client.
Rx Bytes | Shows the total size of the packets received from the client.
Rx Drop Packets | Shows the number of received packets which were discarded.
Rx Drop Bytes | Shows the number of received bytes which were discarded.

> Note

> > "Noise Level", "SNR", "Transmit Packets Discarded", "Transmit Bytes Discarded", "Received Packets Discarded" and "Received Bytes Discarded" are not supported in this version.

### Client Definition List

With this list, you can define display names and notes for specific clients to help with identification in the Associated Client View.
The client names will be used only in the Associated Client View and Associated Client History View. The IDS/IPS Report and Management Log screens will not be affected.

Section 1

Table 18
Item Name | Description
--- | ---
"Export as CSV file" button | Exports registered client definition to a CSV (Comma-Separated Values) format file.
"Import from CSV file" button | The "Import from CSV" dialog box will appear. "Select File" button: Opens a file dialog box to specify a CSV file. The CSV file must contain the following data: * Lines starting with "#" are ignored. 1st column: MAC Address 2nd column: Client Name 3rd Column: Note Note Only CSV format is supported for import. "Add" button: Register client definitions from the specified CSV file. "Cancel" button: Don't import from a CSV file.
"Add" button | Shows the "Add client definition" dialog box. MAC Address: Enter the MAC address of the client. Name: Enter a display name to show in the "Associated Client View" or "Associated Client History View". Notes: Enter a comment. "OK" buttton: Saves the client definition. "x" button: Stops the client definition.

Section 2

Table 19: Client Definition List
Item Name | Description
--- | ---
X Client definition | Shows the total number of client definition entries.
Search client definition | Lets you search client definition entries. The Search field lets you enter a partial string to match. The screen displays entries with that string in one of the following fields: "Name" or "Notes". To remove the filter, delete the string from the Search field and press Enter. Note The search is case-sensitive.
MAC Address | Shows the defined MAC address.
Client Name | Shows the defined display name of the client.
Notes | Shows any comments you entered about the client definition.
Edit (pencil icon) | Shows the "Add client definition" dialog box. MAC Address: Enter the MAC address of the client. Name: Enter a display name to show in the "Associated Client View" or "Associated Client History View". Notes: Enter a comment. "OK" buttton: Saves the client definition. "x" button: Stops the client definition.
Delete (trashbin icon) | Deletes the client definition.

### Associated Client History View

In the Associated Client View, by checking "Associated Client History View", you can view only clients that were associated with the APs on the floor map during the specified time period.
If AWC has stored estimates of an associated client's location, then this view shows the client's past locations. This is called the Associated Client Location Estimation History display. If AWC does not have past estimates of an associated client's location, then this view shows the changes in affiliation. This is called the Associated Client Roaming History display. These display optiions may be mixed, so that the screen shows a mix of location estimation and affiliation display for connected clients.

#### Associated Client Location Estimation History

> Note

> > The Client Location Estimation View will be supported in an upcoming release.

The position is estimated every minute from the radio of the associated client and displayed.
This display appears when all of the following conditions are met in the time period specified:

- The wireless client has connected to a Blanket VAP.
- The system setting "Associated Client Location Estimation History" is enabled.
- Location information is calculated at least once by Associated Client Location Estimation.

If any of these conditions are not met, Client Association Roaming History will be displayed instead.

> Note

> > When using the Client Location Estimation View, set the floor map dimensions (vertical / horizontal) correctly and match AP placement with the actual environment.

> Note

> > System clocks on all the managed APs and the server running the AWC Plug-in must be synchronized.

Section 1

Shows the wireless clients that have been connected to the AP on the map.
When you enter a maximum trace count and select a client from the list, the position of that client is drawn on the floor map.
The client's radio wave will be observed by the APs on the floor every minute, and if enough samples to calculate the location are obtained, the AWC plug-in will calculate the estimated location. The calculation may take several minutes after each observation.
Each estimated location is represented by a circle. The color of the circle represents the reliability of the location estimation (see the legend).
The order and direction of the movement are shown as a broken curve and an arrow head. The curve does not necessarily show the exact path the client moved.
You can hover over each circle to see estimation information as a popup balloon.

Table 20: Client Location Estimation Information
Item Name | Description
--- | ---
Name | Shows the Client Name if defined in the Client Definition List dialog box.
MAC Address | Shows the MAC address of the client.
Notes | Shows any comments entered in the "Client Definition List" dialog box.
Detected Time | Shows the time the client estimation location was detected.
Area Name | Shows the Area Name if the estimated client location is inside an area that has been defined on the "Edit Area" screen.
Estimation Location | Shows the coordinates on the grid of the floor map which the client is estimated to be in. The coordinates origin is the top lefthand corner, starting with "(0,0)".
Reliability | Shows the reliability, as the possible difference between the estimation and actual location, in metres.

Section 2

In the Client History List, "Refresh Timer" is disabled.

Table 21: Floor Map Associated Client Location Estimation History List
Item Name | Description
--- | ---
Details | You can click to see Client Name and Notes, in addition to the default items of MAC Address and Hops. Clicking Details again returns you to the default non-detailed view.
X Client | Shows the number of clients that had been connected to the AP on the floor map during the specified time period.
Search Associated Clients | Entries in the list can be filtered by entering a partial string in the search box. The Search field lets you enter a partial string to match. The screen displays entries with that string in the "MAC Address" field. To remove the filter, delete the string from the Search field and press Enter. Note The search is case-sensitive.
Time Search (Start/End) | Specify a time period with start and end date/time. You can enter a date in "YYYY-MM-DD hh:mm" format or select a day on the calendar that appears when you click the field.
Maximum Trace Count | Specify the maximum number of hops to show. Only the specified number of the most recent hops will be displayed for each client.
Search | Search for clients from the list of clients that were connected to the AP on the floor map during the specified time period.
Associated Client
Checkbox | Lets you select wireless clients to be shown on the floor map. When you check a client, an icon, MAC address, and the position of the client are shown on the map. The latest estimated location is represented as the Client Icon (the laptop shape), and each older location estimation is drawn as a circle. The client's estimated trace is also depicted by a broken line. You can click on an icon on the floor map to see the probable circle based on the estimation reliability. You can hover over the icon to see the location estimation information.
MAC Address | Shows the MAC address of the wireless client.
Hops | Shows the number of estimation entries in the history.

Section 3

Shows the legend for the Associated Client View.
The color of each cell in the legend represents the reliability of the location estimation of clients shown on the map.
The legend can be made invisible or visible by using a checkbox in the floor map control section at the bottom of the page.

Section 4

In the Associated Client View, "Drawing Mode", "Healthiness Icon", and "Power Limit" are irrelevant and disabled.

Table 22: Floor Map Control
Item Name | Description
--- | ---
Grid | Lets you enable or disable grid lines on the floor map. Checking this shows grid lines on the floor map.
Legend | Lets you enable or disable the legend. Check to display.
Details | Whether to display the Associated Client List. Check to display. Check to display.
Floor Area | If areas have been created on the floor map (using the Edit Area page), whether to display the areas. Check to display.
Opacity | Specify the opacity of the floor map background image.

#### Associated Client Roaming History

If the associated client has never met the conditions for showing Associated Client Location Estimation History, and therefore has no location estimation history entries, the Client Association Roaming History will be displayed instead.

Section 1

Shows the wireless clients that have been connected to the AP on the map.
When you check a client in the list, the floor map shows the history of the APs the selected client had connected to in the past.

Section 2

In Client Association Roaming History List, "Refresh Timer" is disabled.

Table 23: Floor Map Client Assoociation Roaming History List
Item Name | Description
--- | ---
Details | You can click to see Client Name and Notes, in addition to the default items of MAC Address and Hops. Clicking Details again returns you to the default non-detailed view.
X Client | Shows the number of clients that had been connected to the AP on the floor map during the specified time period.
Search Associated Clients | Entries in the list can be filtered by entering a partial string in the search box. The Search field lets you enter a partial string to match. The screen displays entries with that string in the "MAC Address" field. To remove the filter, delete the string from the Search field and press Enter. Note The search is case-sensitive.
Time Search (Start/End) | Specify a time period with start and end date/time. You can enter a date in "YYYY-MM-DD hh:mm" format or select a day on the calendar that appears when you click the field.
Maximum Trace Count | Specify a maximum hop counts for each client to show on the map. When you specify the limit, only the specified number of the latest hops will be displayed for each client.
Search | Search for clients from the list of clients that roamed between the APs on the floor map during the specified time period.
Associated Client
Checkbox | Lets you select wireless clients to be shown on the floor map. When you check a client, an icon and the MAC address of the client are shown near the AP to which the client is associated. If the selected client roamed mutiple times between the APs on the map during the specifed time period, its most recent hop in the roaming history will be shown by the client icon. Earlier positions will be shown by circles. The client's roaming trace will be also depicted by a broken line. You can also see when the client was connected to the AP at the position by clicking a client icon or circles. Note The position of the icon does not represent the exact location of the client at the time. Icons are placed so they do not overlap with other icons in the history.
MAC Address | Shows the MAC address of the wireless client.
Hops | Shows how many times the client roamed between APs in the area.

Section 3

Shows the legend for the Associated Client View.
Not used in the Client Association Roaming History View.

Section 4

In the Associated Client View, "Drawing Mode", "Healthiness Icon", and "Power Limit" are irrelevant and disabled.

Table 24: Floor Map Control
Item Name | Description
--- | ---
Grid | Lets you enable or disable grid lines on the floor map. Checking this shows grid lines on the floor map.
Legend | Lets you enable or disable the legend. Check to display.
Details | Whether to display the Associated Client List. Check to display. Check to display.
Floor Area | If areas have been created on the floor map (using the Edit Area page), whether to display the areas. Check to display.
Opacity | Specify the opacity of the floor map background image.

#### Associated Client History (Detail)

Clicking "Details" at the top of the client list in "Associated Client Location Estimation History" or "Client Association Roaming History" extends the list and shows additional information, if that information was provided when the client was defined.

In Associated Client History List, the "Refresh Timer" is disabled.

Table 25: Associated Client History List (Detail)
Item Name | Description
--- | ---
Details | You can click to see Client Name and Notes, in addition to the default items of MAC Address and Hops. Clicking Details again returns you to the default non-detailed view.
X Client | Shows the number of clients connected to the AP that is selected on the floor map.
Search Associated Clients | Entries in the list can be filtered by entering a partial string in the search box. The Search field lets you enter a partial string to match. The screen displays entries with that string in the "MAC Address" field. To remove the filter, delete the string from the Search field and press Enter. Note The search is case-sensitive.
"System Info" / "Wireless Info" / "Statistics" buttons | Switches the contents of the list.
Time Search (Start/End) | Specify a time period with start and end date/time. You can enter a date in "YYYY-MM-DD hh:mm" format or select a day on the calendar that appears when you click the field.
Maximum Trace Count | Specify the maximum hop count (location estimation or roaming counts) to show on the map for each client. When you specify the hop limit, only the specified number of the latest hops will be displayed for each client.
Search | Search for clients from the list of clients that were connected to the AP on the floor map during the specified time period.
Checkbox | Lets you select wireless clients to be shown on the floor map. When you check a client, an icon and the MAC address of the client are shown near the AP to which the client is associated. If the selected client roamed mutiple times between the APs on the map during the specifed time period, its most recent hop in the roaming history will be shown by the client icon. Earlier positions will be shown by circles. The client's roaming trace will be also depicted by a broken line. You can also see when the client was connected to the AP at the position by clicking a client icon or circles. Note The position of the icon does not represent the exact location of the client at the time. Icons are placed so they do not overlap with other icons in the history.
MAC Address | Shows the MAC address of the wireless client.
Hops | Shows how many times the client had its location estimated or had roamed between APs on the Map.
Client Name | Shows the Client Name if defined in the "Client Definition List" dialog box.
Notes | Shows any comments entered in the "Client Definition List" dialog box.

## Floor Map [Smart Connect View]

When AWC-SC (unsupported feature) Smart Connect Network is configured on the floor map, you can see an overview of the connection status, the AP roles, and so on.

Section 1

- The wireless AP icons indicates the roles in AWC-SC.
  - Root AP:
    Indicated by a wired AP icon.

  - Satellite AP (Connector AP or Terminator AP)
    Indicated by an icon of the AP connected by radio.

  Note that the icons will display as follows if the definition in the SC Profile and the actual behavior are inconsistent:
  - Acting as a Satellite AP in spite of being defined as a Root AP
    The UTP cable may be not wired up.

  - Acting as a Root AP in spite of being defined as a Satellite AP
    A UTP cable may be still connected unintentionally.

  - Not acting as an AWC-SC member AP
    The AP may not be under management, the firmware may not be up to date, or the required license may not have been applied.

- You can see the logical connections between the wireless APs, by selecting "Topology" from the "Drawing Mode" dropdown menu in the floor map control, at the bottom of the contents section.
  In Topology drawing mode, the link between wireless APs is drawn with a gray line.
  When the "Healthiness Icon" in the floor map control is checked, the radio wave strength will be indicated by the number of ripples in the balloon of the Healthiness Icon.

  Table 26: Healthiness Icons
  Number of ripples | Power
  --- | ---
  | 4 | -57dBm or greater
  | 3 | -67 to -58dBm
  | 2 | -80 to -68dBm
  | 1 | -90 to -81dBm
  | 0 | -94 to -91dBm

- You can see the traffic utilization between the wireless APs, by selecting "Traffic" from the "Drawing Mode" dropdown menu in the floor map control, at the bottom of the contents section.
  In the Traffic utilization drawing mode, the link line is divided in the middle, and each half depicts the utilization rate from the AP linked directly; for example in the link between AP1 and AP2, the half link nearer to AP1 shows the transmission utilization rate from AP1 to AP2, and the half nearer to AP2 shows transmission from AP2 to AP1.

  The color of the half link indicates the utilization rate.
  The utilization rate is calculated based on the link speed betweeen the APs.
  - Light blue: 0 to 25%
  - Green: 25 to 50%
  - Yellow: 50 to 75%
  - Red: 75 to 100%

Section 2

Table 27: Smart Connect AP List
Item Name | Description
--- | ---
Details | Clicking this shows Acceptor and Connector Tx / Rx Bytes per second and tags, in addition to the default items (Device Name, SC Status, and MAC Address). Clicking Details again returns you to the default non-detailed view.
X AP | Shows the number of wireless APs placed on the floor map. This includes APs on which Smart Connect is not enabled or available.
Refresh Timer | Shows the status of the timer that automatically refreshes the page. The blue portion of the bar shows the elapsed time since the last refresh and the grey or white portion shows the time to the next refresh. The list is automatically refreshed at the interval configured on "Refresh Rates" > "Floor MAP (Smart Connect)" in the User Management menu. (The default is 5 seconds.)
Search Wireless AP | The Search field lets you enter a partial string to match. The screen displays entries with that string in one of the following fields: "Device Name", "SC Status", or "MAC Address" fields. To remove the filter, delete the string from the Search field and press Enter. Note The search is case-sensitive.
Device Name | Shows the name given to the AP.
SC Status | Shows the AP's role in AWC-SC. Root: This AP acts as a Root AP, which is a bridge for the traffic between the wired backbone network and the devices in the fronthaul, such as clients, Connector APs or Terminator APs. Connector: This AP acts as a Connector AP, which is a bridge for the traffic between the Root AP in the backhaul and the clients or Terminator APs in the fronthaul. Terminator: This AP acts as a Terminator AP, which is a bridge for the traffic between the clients in the fronthaul and the Root or Connector APs in the backhaul. Unknown: The AWC-SC connection is not established. Alternatively, Smart Connect is not enabled on the AP.
MAC Address | Shows the device's MAC address.

Section 3

Shows the legend for Smart Connect Traffic drawing mode.
The color of each cell in the legend represents the utilization rate between the APs on the map.
The legend can be made invisible or visible by using a checkbox in the floor map control section at the bottom of the page.

Section 4

In the Smart Connect View, "Power Limit" is irrelevant and disabled.
Also, when the drawing mode is "Topology", "Legend" will be disabled, and when the drawing mode is "Traffic", the "Healthiness Icon" will be disabled.

Table 28: Floor Map Control
Item Name | Description
--- | ---
Drawing Mode | You can select the mode that the link lines between APs on the floor map represent, either "Topology" or "Traffic".
Grid | Lets you enable or disable grid lines on the floor map. Checking this shows grid lines on the floor map.
Legend | Lets you enable or disable the legend. Check to display.
Details | Toggles the visibility of the AP List. Check to display.
Healthiness Icon | In Topology drawing mode, whether to display the Healthiness Icon. Check to display.
Floor Area | If areas have been created on the floor map (using the Edit Area page), whether to display the areas. Check to display.
Opacity | Specify the opacity of the floor map background image.

### Smart Connect AP List (Detail)

Clicking "Details" at the top of the AP list in the "Smart Connect View" extends the list to show additional information such as SC Status and Tx / Rx throughput.

Table 29: Floor Map Smart Connect View AP List (Detail)
Item Name | Description
--- | ---
Details | Clicking this shows Acceptor and Connector Tx / Rx Bytes per second and tags, in addition to the default items (Device Name, SC Status, and MAC Address). Clicking Details again returns you to the default non-detailed view.
X AP | Shows the number of wireless APs placed on the floor map. This includes APs on which Smart Connect is not enabled or available.
Refresh Timer | Shows the status of the timer that automatically refreshes the page. The blue portion of the bar shows the elapsed time since the last refresh and the grey or white portion shows the time to the next refresh. The list is automatically refreshed at the interval configured on "Refresh Rates" > "Floor MAP (Smart Connect)" in the User Management menu. (The default is 5 seconds.)
Search Wireless AP | You can search for wireless APs on the floor map. The Search field lets you enter a partial string to match. The screen displays entries with that string in one of the following fields: "Device Name", "SC Status", or "MAC Address" fields. To remove the filter, delete the string from the Search field and press Enter. Note The search is case-sensitive.
Device Name | Shows the name given to the AP.
SC Status | Shows the AP's role in AWC-SC. Root: This AP acts as a Root AP, which is a bridge for the traffic between the wired backbone network and the devices in the fronthaul, such as clients, Connector APs or Terminator APs. Connector: This AP acts as a Connector AP, which is a bridge for the traffic between the Root AP in the backhaul and the clients or Terminator APs in the fronthaul. Terminator: This AP acts as a Terminator AP, which is a bridge for the traffic between the clients in the fronthaul and the Root or Connector APs in the backhaul. Unknown: The AWC-SC connection is not established. Alternatively, Smart Connect is not enabled on the AP.
MAC Address | Shows the device's MAC address.
Acceptor Tx | Shows the throughput of the traffic transmitted to the fronthaul AP (Terminator AP for Root/Connector APs, and Connector AP for Root AP) in bytes per second.
Acceptor Rx | Shows the throughput of the traffic received from the fronthaul AP (the Terminator AP for Root/Connector APs, and the Connector AP for the Root AP) in bytes per second.
Connector Tx | Shows the throughput of the traffic transmitted to the backhaul AP (the Root AP for Connector/Terminator APs, and the Connector AP for the Terminator AP) in bytes per second.
Connector Rx | Shows the throughput of the traffic received from the backhaul AP (the Root AP for Connector/Terminator APs, and the Connector AP for the Terminator AP) in bytes per second.
Tag | Shows the tags set on the AP.

## Floor Map [Rogue AP View]

Section 1

- Managed AP icons turn red on the map if there are rogue AP detection reports by the managed AP during the time period specified in section 2.
- Clicking a managed AP on the map toggles display status of the detected rogue APs.

  > Note

  > > The position of the rogue AP icon does not represent the exact location of the rogue AP at the time. Icons are placed to not overlap with other icons in the history.

- When you click a rogue AP icon on the floor map, the corresponding entry in section 2 is highlighted.

Section 2

In Rogue AP View, "Refresh Timer" is disabled.

Table 30: Floor Map Rogue AP List
Item Name | Description
--- | ---
Details | Clicking this shows the reason to consider the detected neighbor AP a rogue, the SSID, Channel and detecting AP, in addition to the default items (BSSID, RSSI and Detection Time).. Clicking Details again returns you to the default non-detailed view.
X ROGUE | Shows the number of rogue APs that match the specified time period and received signal strength.
Date/Time | Specify a date and time, to filter rogue APs on the list. You can enter a date in "YYYY-MM-DD hh:mm" format or select a day on the calendar that appears when you click the field. The time can be selected in one-hour intervals. Alternatively, a slider control lets you specify a more granular time.
Search | Filters rogue AP detection history by the specifed date/time.
Threshold Filter | Specify a minimum received signal strength for a rogue AP to be displayed. Rogue APs are only shown on the list and floor map if the received signal strength of the rogue AP is greater than the specified minimum value.
Slider Control | Lets you specify detection time in 5 minute intervals.
Rogue AP List
Detected BSSID | Shows a list of BSSIDs that managed APs on the map detected. Clicking a rogue AP entry in the list toggles display of all rogue AP icons detected by the managed APs. When the display status of a rogue AP icon is enabled, you can highlight the rogue AP's icon on the floor map by hovering over the rogue AP entry in the list.
RSSI | Received Signal Strength of the rogue AP observed on the detecting managed AP. A higher value (closer to 0) means a stronger signal, therefore the rogue AP may be closer to the detecting managed AP.
Detected Time | Shows the date/time when the managed AP detected the rogue AP.

Section 3

In the Rogue AP View, "Drawing Mode", "Legend", "Healthiness Icon", and "Power Limit" are irrelevant and disabled.

Table 31: Floor Map Control
Item Name | Description
--- | ---
Grid | Lets you enable or disable grid lines on the floor map. Checking this shows grid lines on the floor map.
Details | Toggles the visibility of the Rogue AP List. Check to display.
Floor Area | If areas have been created on the floor map (using the Edit Area page), whether to display the areas. Check to display.
Opacity | Specify the opacity of the floor map background image.

### Rogue AP List (Detail)

Clicking "Details" at the top of the Rogue AP list on "Floor Map [Rogue AP View]" extends the list to show additional information such as Rogue Reason, SSID, Channel and Detecting AP.

Table 32: Floor Map Rogue AP List (Detail)
Item Name | Description
--- | ---
Details | Clicking this shows the reason to consider the detected neighbor AP a rogue, the SSID, Channel and detecting AP, in addition to the default items (BSSID, RSSI and Detection Time).. Clicking Details again returns you to the default non-detailed view.
X ROGUE | Shows the number of rogue APs that match the specified time period and received signal strength.
Search Rogue AP | Entries in the list can be filtered by entering a partial string in the search box. The Search field lets you enter a partial string to match. The screen displays entries with that string in one of the following fields: "BSSID" or "SSID". To remove the filter, delete the string from the Search field and press Enter. Note The search is case-sensitive.
Date/Time | Specify a date and time, to filter rogue APs on the list. You can enter a date in "YYYY-MM-DD hh:mm" format or select a day on the calendar that appears when you click the field. The time can be selected in one-hour intervals. Alternatively, a slider control lets you specify a more granular time.
Search | Filters rogue AP detection history by the specifed date/time.
Threshold Filter | Specify a minimum received signal strength for a rogue AP to be displayed. Rogue APs are only shown on the list and floor map if the received signal strength of the rogue AP is greater than the specified minimum value.
Slider Control | Lets you specify detection time in 5 minute intervals.
Filter by tag | Lets you filter APs with tags. Clicking tags uses the tags to filter the list. Clicking them again removes the filter. Clicking "Clear filter" removes the filter for all tags.
Rogue AP List
Rogue Reason | Shows the reason to consider the detected neighbor AP a rogue.
Detected BSSID | Shows a list of BSSIDs that managed APs on the map detected.
SSID | Shows the SSID of the detected AP.
RSSI | Received Signal Strength of the rogue AP observed on the detecting managed AP. A higher value (closer to 0) means a stronger signal, therefore the rogue AP may be closer to the detecting managed AP.
Detecting AP | Shows the AP name which detected the neighbor AP.
Detected Time | Shows the date/time when the managed AP detected the rogue AP.
Tag | Shows tags added to the AP.

## Floor Map [Add AP to Map]

In this view, you can place an AP on the floor map.

Section 1

- When you click the row of the AP you want to place on the Map from the list of unallocated APs in Section 2, the mouse pointer changes to the wireless AP icon.
  By clicking on the grid of the floor map with the icon, you can place the AP on the floor map.
- The status of the placed AP will be displayed on the floor map, depending on what you previously selected in the View Selection dropdown menu. If you selected "Smart Connect View" in the dropdown menu, you will see the AP's Smart Connect status, and if you selected a different view, the AP status will be drawn on the floor map according to the "Wireless Status View".
- If you want to move an AP icon on the floor map, you can drag and drop it on the place you want it to move to.
- To remove an AP icon on the floor map, click on it to select it (the selected icon will drawn with a blue circle behind it) and then click the "Delete from Map" button at the top right of the content section.
  You can select multiple APs by clicking them one by one.
  To deselect, click on the "Unselect" button at the top right of the content section.

The changes (placement, relocation, and removal) on the floor map will be saved immediately.

Section 2

Shows the wireless AP list.
The list contains only the APs that belong to the same Management Group as the map, and that are not yet placed on any map.

Table 33: Floor Map Unallocated AP List
Item Name | Description
--- | ---
X AP | Displays the number of wireless APs under the management group to which the floor map belongs, that are not yet placed on any floor map.
Search Wireless AP | You can search for wireless APs not placed on the floor map. The Search field lets you enter a partial string to match. The screen displays entries with that string in one of the following fields: "Management Status", "Device Name", "IP address", or "AP Profile". To remove the filter, delete the string from the Search field and press Enter. Note The search is case-sensitive.
Device Name | Shows the name given to the AP.
Status Icon | When the AP is managed by the AWC Plug-in, a green checkmark is displayed. When the AP is not managed by the AWC Plug-in, a red triangle is displayed.
Management Status | Shows the Management Status of the AP.
IP Address | Shows the AP's IP address.

Section 3

Shows the legend of either the Wireless Status View or Smart Connect View.
The legend will be shown according to the immediately previous selection of the Views; the Smart Connect View legend for Smart Connect View, and the Wireless Status View legend for the others.

Section 4

The legend will be shown according to the immediately previous selection of the Views; the Smart Connect View legend for Smart Connect View, and the Wireless Status View legend for the others.

Table 34: Floor Map Control
Item Name | Description
--- | ---
Drawing Mode | The options in the Drawing Mode dropdown menu differ according to the immediately previous selection of the Views. If you chose Smart Connect View previously, the Drawing Mode dropdown comes with Topology and Traffic, and if you chose another view, the dropdown comes with Power and Channel.
Grid | Lets you enable or disable grid lines on the floor map. Checking this shows grid lines on the floor map.
Legend | Lets you enable or disable the legend. Check to display.
Details | Whether to display List of unallocated APs. Check to display.
Healthiness Icon | Whether to display the Healthiness Icon. This will work if you chose Smart Connect View from the View Selection dropdown menu immediately before, and you chose Topology from the Drawing Mode. Otherwise, this is irrelevant and disabled. Check to display.
Floor Area | If areas have been created on the floor map (using the Edit Area page), whether to display the areas. Check to display.
Power Limit | You can set the lower limit of the wireless strength that is drawn on the heat map display, if you chose a view other than Smart Connect View from the View Selection dropdown menu immediately before.
Opacity | Specify the opacity of the floor map background image.

## Floor Map [Edit Area]

You can draw areas (rooms, etc.) with planar polygons, and name these areas such as "Meeting Room", "Lounge", and "Auditorium" on the floor map.
The defined areas will be displayed in each View of the floor map, and also shown in the Location Estimation popup information in the Associated Client View.

Section 1

You can view and draw areas.

- Start by drawing an area on the map, as a polygon or rectangle. The colors of the areas are not configurable manually but are chosen randomly.
  Enter an "Area Name" and click on the "Add" button to save the area you drew on the map.
- When you hover over an existing area, a popup balloon shows the area name.
- By clicking on an area, you can edit it.
  - You can reshape it by drag-and-drop on each corner point.

    > Note

    > > You can not add or delete corner points.

  - Edit "Area Name" to change the area name.
  Click "Save" to save the changes to the name and shape.

> Note

> > Areas must be drawn so that they do not overlap. For example, to create an area that surrounds another area, such as a corridor, divide the area into two or more areas.
> > If areas overlap, the Client Location Estimation display might become inaccurate.

Section 2

Shows the Area list.

Table 35: Floor Map Area List
Item Name | Description
--- | ---
X Area | Shows the number of areas defined on the floor map.
Area Name | The area name displayed in the "Associated Client View".
"Add" / "Save" button | Saves a newly created area or edited existing area. You can create a new area by drawing a polygon or a rectangle on the floor map, entering Area Name, and clicking on the "Add" button.
"Clear" / "Cancel" button | Cancels changes before clicking the "Add" / "Save" button.
"Simple Create Mode" vs "Normal Create Mode" radio button | Switches the drawing mode of the area. Do not confuse with the Drawing Mode of Views such as Channel and Power, or Topology or Traffic. The default is "Simple Create Mode". Simple Create Mode: You can draw the area as a rectangle. At one of the corners you are going to draw, hold down the left mouse button, then drag to the opposite corner of the rectangle, and release. You can drag and drop corners or sides to adjust the position or the size, as long as you do not click the "Add" button. Once you have saved the area, the shape will be treated as a polygon with four corner points, that is, you can not drag the sides to reshape it if you edit it again. Normal Create Mode: You can draw an area as a polygon. Click the corners to draw them one by one, and double-click on the first corner point to close the polygon. You can drag and drop corners to reshape the area. Once you close the path, you can not add or delete corner points.
Search Floor Areas | You can search for areas defined on the floor map. The Search field lets you enter a partial string to match. The screen displays entries with that string in the "Area Name" field. To remove the filter, delete the string from the Search field and press Enter. Note The search is case-sensitive.
Area Name | Shows the area name defined for display.
"Edit" button | Enters edit mode for the selected area.
"Copy" button | Duplicates the selected area. The Area Name of the duplicated area will be the original Area Name plus "_copy". If this name is already in use, a sequential number with brackets follows the suffix, such as "_copy(1)". The duplicated area polygon will be the same shape and will be placed at the top left of the map. Move and reshape it as needed.
"Delete" button | Deletes the selected area.

Section 3

On the Edit Area screen, "Drawing Mode", "Legend", "Healthiness Icon", and "Power Limit" are irrelevant and disabled.

Table 36: Floor Map Control
Item Name | Description
--- | ---
Grid | Lets you enable or disable grid lines on the floor map. Checking this shows grid lines on the floor map.
Details | Toggles the visibility of Area List. Check to display.
Floor Area | If areas have been created on the floor map (using the Edit Area page), whether to display the areas. Check to display.
Opacity | Specify the opacity of the floor map background image.

13 Mar 2020 16:32