User Guide: Vista Manager AWC Plug-in version 3.16.0

# Configure Floor Maps

This section covers the procedures to create, edit, and delete floor maps.
Floor Maps let you create a location map of the managed APs and facilitate AP management tasks.
They also visualize radio signal strength and coverage with the heatmap function that shows signal strength with colors.

> Note

> > The heatmap calculates the radio signal strength at a given point from an AP's transmit power and the distance between the AP and the point. Because it assumes that there are no obstacles and reflection between the AP and the point, the actual radio signal strength may differ from the heatmap's calculation.

> Note

> > A single floor map supports 120 APs and 20 tags.

> Note

> > If you manage 1001 or more APs, use 160 or less floor maps.

> Note

> > If you place many APs on a large floor map, it may take time to load the floor map, or to place APs on the map.

## Create Floor Map

1. Select "Wireless Monitoring" > "Floor Map" from the AWC Plug-in menu.
2. Click "Create" at the top right corner.
3. The "Create Deployment Map" dialog box will appear.

   Table 1: "Create Deployment Map" dialog box
   Item Name | Description
   --- | ---
   Map Name | Enter a name for the Floor Map. Should be 1 to 100 characters in length, with alphabets, numbers and symbols (including spaces).
   Background image | Specify a background image for the Floor Map. Supported formats are JPEG, PNG, and GIF, with the filesize up to 4MB. Note An error may not be displayed even when you specify an unsupported file (a file in formats other than PNG, JPEG, or GIF) with a size larger than 4MB. Animated GIFs are not supported. It will be displayed as a still image if specified. Note A map image with a margin around the floor makes the floor size calculation less accurate. We recommend that you trim the margin on the image with an image editor.
   Floor width / Floor height | Specify an actual size (width and height) of the installation site within the range of 10 to 1000 (in meters). When you enter either width or length, the other value is automatically filled in according to the aspect ratio of the image. Floor size affects the heat map and the location estimation of connected clients in the Wireless Status View. Note The Location Estimation function will be supported with TQ6602 GEN2, TQ6702 GEN2 firmware version 8.0.3-0.x or later; or with TQ5403, TQ5403e firmware version 6.0.1-1.x or later.
   Management Group | Specify a management group for the map.
   Tag | Enter a tag of your choice and press the Enter key. A single tag can contain up to 100 alphanumeric characters and symbols (including spaces), excluding consecutive spaces and line breaks. A single map can contain 20 tags. To delete a tag, click "x" to the right of the tag. Note If you paste a tag string from the clipboard, not all text may be visible. In that case, press Enter to make a tag from the entire pasted string. Note Pasting a tag containing a newline is not supported. Note Tag names may be truncated in the tag filter list on the Devices Map, Floor Map Details and Device Search pages. To avoid this, use shorter names for the tags.
   Notes | Enter a comment. It will be displayed in a balloon when you mouse over the map in the Floor Map panel or list. Comments can contain up to 1,000 alphanumeric characters and symbols (including spaces), excluding consecutive spaces and line breaks.
   "Add" button | Create the map.
   "Cancel" button | Cancels creating the map.

4. When you have entered all required information for the floor map, click "Add".

## Edit Floor Map

1. Select "Wireless Monitoring" > "Floor Map" from the AWC Plug-in menu.
2. Mouse over a floor map panel.
   The "Edit" button (pencil icon) will appear at the top right of the Floor Map panel.
3. Click the "Edit (pencil)" button to display the "Edit Deployment Map" dialog box.

   Table 2: "Edit Deployment Map" dialog box
   Item Name | Description
   --- | ---
   Map Name | Enter a name for the Floor Map. Should be 1 to 100 characters in length, with alphabets, numbers and symbols (including spaces).
   Background image | Specify a background image for the Floor Map. Supported formats are JPEG, PNG, and GIF, with the filesize up to 4MB. Note An error may not be displayed even when you specify an unsupported file (a file in formats other than PNG, JPEG, or GIF) with a size larger than 4MB. Animated GIFs are not supported. It will be displayed as a still image if specified. Note A map image with a margin around the floor makes the floor size calculation less accurate. We recommend that you trim the margin on the image with an image editor.
   Floor width / Floor height | Specify an actual size (width and height) of the map in meters. When you enter either width or length, the other value is automatically filled in according to the aspect ratio of the image. Floor size affects the heat map and the location estimation of connected clients in the Wireless Status View. Note The Location Estimation function will be supported with TQ6602 GEN2, TQ6702 GEN2 firmware version 8.0.3-0.x or later; or with TQ5403, TQ5403e firmware version 6.0.1-1.x or later.
   Management Group | Specify a management group for the map.
   Tag | Enter a tag of your choice and press the Enter key. A single tag can contain up to 100 alphanumeric characters and symbols (including spaces), excluding consecutive spaces and line breaks. A single map can contain 20 tags. To delete a tag, click "x" to the right of the tag. Note If you paste a tag string from the clipboard, not all text may be visible. In that case, press Enter to make a tag from the entire pasted string. Note Pasting a tag containing a newline is not supported. Note Tag names may be truncated in the tag filter list on the Devices Map, Floor Map Details and Device Search pages. To avoid this, use shorter names for the tags.
   Notes | Enter a comment. It will be displayed in a balloon when you mouse over the map in the Floor Map panel or list. Comments can contain up to 1,000 alphanumeric characters and symbols (including spaces), excluding consecutive spaces and line breaks.
   "Add" button | Create the map.
   "Cancel" button | Closes the dialog box without saving changes.

4. Click the "Save" button to save the changes.

## Delete Floor Map

> Note

> > Even if you delete all entries on the last page of the list, the page will not be deleted and an empty list page will be displayed. The number of pages will be refreshed after moving to another page or reloading the browser.

1. Select "Wireless Monitoring" > "Floor Map" from the AWC Plug-in menu.
2. Mouse over a floor map panel.
   The "Delete" button (trashbin icon) will appear at the top right of the Floor Map panel.
3. Click the "Delete (trashbin)" button to display a confirmation dialog box.
4. Click "Delete".

11 Feb 2026 14:56