User Guide: Vista Manager AWC Plug-in version 3.6.0

# Create SC Profile

Next let's create SC Profiles for Smart Connect networks.
SC Profile consists of the following items.

- Profile Configuration
  Select the model of the AP or the Management Group to be applied.
- Basic Configuration
  Create a SC Management VAP to use instead of a wired connection.
- Wireless Configuration
  Select radio band and channel including SC VAP.
- AP List
  Select the AP that uses Smart Connect and the AP that is used as the Root AP from the APs belonging to the Management Group.

1. Select "Wireless Configuration" > "SC Profile" from the AWC Plug-in menu.
   This shows a list of SC Profiles.

2. Click "Create" at the top right corner.
   The "Create SC Profile" dialog will appear.

3. Enter a name for the SC Profile.
   Here, enter "TQ5403SC".
4. Select a Country.
   If the default country code for the currently logged in user is configured, it is selected by default.
5. Select the AP model that uses Smart Connect.
   Here, Select only "AT-TQ5403". The selected model name is displayed in blue.
6. Select the management group to which the SC Profile applies.
   One SC Profile can be created for one Management Group.
   Here, we select "3F Group".

7. Set "SSID" in "Basic Configuration" as necessary.
   By default, it is automatically set in the form of "SC-Default-*****". "*****" is a randomly generated 5 alphanumeric characters (mixed case).
   This SSID is not broadcast. Since it is used only between APs set via the AWC Plug-in, there is no special consideration unless it overlaps with multi-channel VAPs, CB VAPs, and other SSIDs for SC management used in the same space.
   Note that even if the beacon broadcast by the AP does not include the SSID, the communication packet will includ the SSID to identify the wireless network. Since it is possible to display the hidden SSID from communication packets by using wireless network monitoring tools, it is recommended to avoid using strings that easily identify your network in order to prevent attacks from malicious users.
   Here, "SC-Default-cVVGG" set by default is used.
   If necessary, click the icon to the right of "Security Key (WPA-PSK)" to check the set character string.
   The security key is a pre-shared key used for the SC management SSID. 63 randomly generated alphanumeric characters (mixed case) are automatically set and cannot be changed.
   The created SSID will overwrite the VAP 1 setting of the Frequency selected in the Radio Configuration.
   Also, when "Auto Discovery" is enabled in the next section, the SSID "sc-initial-provisioning" for connecting the factory default AP to the Smart Connect network occupies VAP 2 in the same band.
   When disabled, "sc-initial-provisioning" is not set for VAP2.
   VAP settings created in the same wireless band with AP Profile are ignored.
8. Select whether to Enable or Disable "Auto Discovery".
   - When set to "Enable", it responds to the connection request from the factory default AP. Enable when adding a wireless AP by OTA (Over The Air).

     > Note

     > > When using Auto Discovery, the network address 172.31.0.0/24 cannot be used on the network.

     > Note

     > > Auto Discovery can be very time consuming. If this is the case, connect the AP directly to the network to which the AWC Plug-in belongs and configure the settings.

   - When set to "Disabled", it does not respond to connection requests from the factory default AP. All Satellite APs (Connector APs / Terminator APs) need to be wired.
   Here, set it to "Enable".

9. In "Selection Type" of "Radio Configuration", select whether to automatically set the channel to use Smart Connect or set it to fixed.
   - When "Auto" is selected, the channel is automatically selected according to "Frequency" and "Bandwidth".

     > Note

     > > If you have selected a specific channel for the radio band that uses AWC-SC in the AP profile, do not set the Selection Type to "Auto" in the SC Profile. When "Auto" is selected, a channel other than the one set in the AP profile may be used.

   - When "Fixed" is selected, the channel number corresponding to "Frequency" is displayed in the "Channel".
   The default is "Auto".
   Here, set it to "Fixed".
10. Select "Frequency" from "2.4 GHz" (Radio 1) and "5 GHz Low" (Radio 2 W52).
    Here, select "5 GHz" because the SSID for SC management and the SSID for the factory default AP connection "sc-initial-provisioning" are created in the "Radio 2".

    > Note

    > > In the radio band used by AWC-SC, the other VAPs will be disabled automatically.

11. Select "Bandwidth".
    Here, select "40MHz".
12. Select "Channel".
    When "Fixed" is selected in "Selection Type", specify the channel used for communication between APs.
    Here, select "36ch"

13. From the "AP List", select the AP that uses Smart Connect.
    The "AP List" displays a list of APs that belong to the selected Management Group.
    By default, Smart Connect is enabled for all APs belonging to the Management Group.
    If there is an AP that does not use Smart Connect in the AP List, click "Enable" (blue) of "Smart Connect" to switch it to "Disable" (gray).
    Here, it is assumed that all registered APs use Smart Connect.

    > Note

    > > In the "AP list", all APs belonging to the same Management Group are displayed, including APs that do not support AWC-SC.
    > > Even if Smart Connect is set to "Enable" for an AP that does not support AWC-SC, it cannot connect to the Smart Connect network.
    > > Additionally, if there are APs that do not support AWC-SC in the Management Group, set Smart Connect to "Disable" in the "AP List" on the "Edit SC Profile" screen. When Smart Connect is set to "Enable" for an AP that does not support AWC-SC, some wireless settings that overlap with the SC profile, such as the channel used, are ignored.

14. From the "AP List", select the AP to use as the Root AP.
    Here, check the "Root" of "TQ5403-SC-1".

    The Root AP can also be selected from the Floor Map.
    Click the "Floor Map" at the top right of the "AP List" to display floor map panels belonging to the Management Group. Click the floor map panel to display the Floor Map dialog, APs on the map are shown graphically.
    Put mouse cursor on an AP, the IP address, MAC address and model name will pop up. Click the wireless AP icon, the Root AP icon will be displayed at the top right of the AP icon. Click the "OK" to close the Floor Map dialog.

15. Click the "Add" button on the top right of the screen.
    SC Profile "TQ5403SC" is registered.

You are done with creating a SC Profile.

15 Jul 2021 12:03