User Guide: AT-RADGate for VST-APL/VST-VRT version 1.0.0

# Status Monitor

Endpoint

The "Status Monitor" page manages the status of devices that have undergone authentication processing by AT-RADgate.

## Endpoint

A list of the status of devices authenticated by AT-RADgate is displayed. This page is provided for the purpose of managing endpoints authenticated by the port authentication function of the AW+ device, and any other operations are not supported.
The device status displayed on this page has the following restrictions.

- Only devices that have been authenticated via a NAS that has been assigned a "NAS Profile" with endpoint authentication enabled is displayed.
- If the RADIUS Accounting settings are not enabled on the NAS, devices that have already left the network continue to be displayed because the device disconnection cannot be detected.
- If RADIUS Accounting packets are lost on the network, endpoints that have already left the network may continue to be displayed.
- If the NAS is restarted, devices connected to it continue to be displayed.

Table 1: Status Monitor
Item Name | Display | Search | Sort | Description
--- | --- | --- | --- | ---
MAC Address | × | × | × | The endpoint's MAC Address.
Status | × | × | × | The status of the device.
VLAN | × | − | × | The destination VLAN.
Device Name | × | × | × | The device name of the device.
Connected NAS IP Address | × | × | × | If authentication is performed via a NAS, the IP Address of the NAS is displayed.

The functions of each button at the top right of the page are as follows:

Table 2: Button Functions
Button Name | Description
--- | ---
Manage Columns | Changes the visibility of each column in the table.
Reload | Reloads the device status list.

Each row in the table has a menu button at the far right that allows you to manage the policies for that row. The functions of each menu are as follows.

Table 3: Button Functions
Button Name | Description
--- | ---
Disconnect | Send a disconnection request to the NAS.

17 Jun 2025 09:28