User Guide: AMF Security mini version 1.7.0

# Welcome to the AMF Security mini User Guide

Allied Telesis Autonomous Management Framework (AMF) simplifies and automates network management. AMF Security mini adds a powerful security component with an intelligent SDN controller that works with firewalls and other security devices to instantly respond to alerts, and block the movement of malware threats within a wired or wireless network.

The Device GUI supports AMF Security mini (AMF-Sec mini) on the AR4050S UTM Firewall.

This requires:

- AR4050S running AlliedWare Plus 5.5.0-0.1 or later and Device GUI 2.5.1 or later
- AMF-Sec mini image file (sesc_mips64_1.7.0.app) installed on the AR4050S

To install and access the AMF Security mini application on your device:

1. Download the image file (sesc_mips64_1.7.0.app) from the Software Download area of the Allied Telesis website and load it into the flash memory on the AR4050S.
2. In the Device GUI’s navigation bar, select Vista Manager mini > AMF Security mini.

From the AMF Security mini page in the Device GUI, you can enable the AMF-Sec mini application and use the wizard to configure storage, memory and network interfaces.

## Structure of this manual

This HTML manual covers the AMF Security mini application features and how to use them. It is split into the following sections:

## Download this manual

Download a copy of this manual in ZIP format.

- User Guide: AMF Security mini version 1.7.0 (download)

After downloading, extract the ZIP file and open index.html in your preferred web browser.

## Related documents

- Product documents for the AR4050S UTM Firewall.
- User documents for Vista Manager mini.

18 Jan 2021 10:56