User Guide: AMF Security mini version 2.2.0

# Group

UnAuth Group List
Add UnAuth Group
Edit Policy
Update UnAuth Group
Edit Policy

Devices that fail normal authentication and that match specific Location and Schedule conditions are called the UnAuth Group, and are connected to a dedicated network.
For more information on UnAuth Group, Refer to Providing Guest Network by UnAuth Group > What is UnAuth Group in Quick Tour.

## UnAuth Group List

This page shows a list of the UnAuth Group registered in AMF Security mini's database.

Table 1: Target columns for search and sort operations
Item Name | Search | Sort
--- | --- | ---
Group ID | × | ×
Enabled | × | ×
Note | × | ×
Number of Policies | × | ×

Table 2: Displayed columns
Item Name | Description
--- | ---
Group ID | ID (Name) of the UnAuth Group.
Enabled | Whether the group is enabled or not.
Note | Arbitrary string (comment) for the Group.
Number of Policies | Number of security policies applied to the group.

Table 3: Buttons
Item Name | Description
--- | ---
Page Top
Add UnAuth Group | Open the Add UnAuth Group page.
Export to CSV | Start downloading of a list of the UnAuth Group in CSV format.
UnAuth Group List
Heading Row
Delete Selected | Delete all the checked groups.
Each Row
Edit | Open the Update UnAuth Group page for the selected group.
Delete | Delete the group.

> Note

> > Refer to Appendix > CSV File for CSV Files.

### Add UnAuth Group

This page lets you add a new UnAuth Group.

Table 4: Sample Configuration Data
Item Name | Description
--- | ---
Enabled | Uncheck this if you want the group to be disabled.
Group ID (Mandatory) | ID (Name) of the group to register. Group ID must be unique. Max 255 characters
Note | Arbitrary string (comment) for the Group. Max 255 characters.
Only detecting the device. | Check this if you want the group to be used only for detecting unregistered devices without allowing them to access the network.

Table 5: Displayed columns
Item Name | Description
--- | ---
Policies
Policies | List of security policies attached to the group.
Priority | A priority value of the security policy. It must be an integer in the range of 0 to 255. When multiple security policies are set, if an interface registered with a device in an UnAuth Group connects to an AMF Member, it is determined whether the security policy with the lowest priority value matches in order.
Network | ID of the network to which AMF Security assigns the device in the group.
Location | Specify a location where the device can be for AMF Security to categorize it in the group.
Schedule | Specify a schedule when the device can be connected for AMF Security to categorize it in the group.

Table 6: Buttons
Item Name | Description
--- | ---
Policies
Heading Row
Add | Open the Edit Policy dialog to add a new security policy for the UnAuth Group.
Each Row
Edit | Open the Edit Policy dialog to edit the selected security policy.
Delete | Mark to delete the security policy attached to the device. The security policy to be deleted is indicated with the DEL mark on the left side of its record line.
Revert | Clear the DEL mark on the security policy.
Page Bottom
Submit | Add a new group with the input information on this page and subordinate dialogs by committing the information for the newly added group.
Cancel | Cancel the operation for adding the new group.

> Note

> > Interfaces and security policies marked with DEL is deleted when the "Submit" button is clicked. Once you click the "Submit" button, you cannot undo the delete operations.

#### Edit Policy

This dialog lets you add a new security policy to the group or update an existing security policy attached to the group.

Table 7: Configurable fields
Item Name | Description
--- | ---
Priority (Mandatory) | A priority value of the security policy. It must be an integer in the range of 0 to 255. When multiple security policies are set, when a device in an UnAuth Group connects to an AMF Member, it is determined whether the security policy with the lowest priority value matches in order.
Network | ID of the network which AMF Security assigns the device to. Maximum 100 IDs of the existing networks are shown in the dropdown list. If you enter text in the field, Network IDs in the dropdown list are dynamically filtered to the ones which contain the input text in Network ID, VLAN ID or Note (it shows maximum 100 elements). From the dropdown list, select a Network ID. If the registered device is connected to AMF Members, it is connected to the VLAN subnet configured in the network. If the network is not registered in the device (if this setting is blank or the VLAN ID is set to 0 in the network security policy setting), it is assigned to the VLAN set as the AMF Member. The connection to the VLAN subnet is realized by sending as a tagged VLAN with the set VLAN ID when it is sent to the upper network of the connected AMF Members. You have to add the network before assigning a device to the network. Refer to Policy Settings > Add Network for the instruction on how to register a network.
Location | Specify a location where the unauthenticated device can be so that it is categorized in the group. Maximum 100 IDs of the existing locations are shown in the dropdown list. If you enter text in the field, location IDs in the dropdown list are dynamically filtered to the ones which contain the input text in Location ID or Note (it shows maximum 100 elements). From the dropdown list, select a Location ID. If you specify Location, the UnAuth Group can access the network only from AMF Members in the location. If you do not specify Location, the UnAuth Group can access the network from all AMF Members. You have to add the location before specifying it for a group. Refer to Policy Settings > Add Location for the instructions on how to add locations.
Schedule | Specify a schedule when the unauthenticated device can be connected to the network so that it is categorized in the group. Maximum 100 IDs of the existing schedules are shown in the dropdown list. If you enter text in the field, Schedule IDs in the dropdown list are dynamically filtered to the ones which contain the input text in Schedule ID or Note (it shows maximum 100 elements). From the dropdown list, select a Schedule ID. If you specify a Schedule, the group can access the network only when the schedule is effective. If you do not specify a schedule, a device can always access the network. You have to add the schedule before specifying it for a group. Refer to Policy Settings > Add Schedule for the instruction on how to register a schedule.

> Note

> > If you can access the VLAN set for AMF Members, depending on the switch settings, the device may be able to connect to devices on the control plane.

Table 8: Buttons
Item Name | Description
--- | ---
Bottom of the dialog
Submit | Add or update the security policy information.
Cancel | Cancel the operation for adding or updating policy.

### Update UnAuth Group

This page lets you update the information of an existing UnAuth Group.

Table 9: Configurable fields
Item Name | Description
--- | ---
Enabled | Uncheck this if you want the group to be disabled.
Group ID (Mandatory) | ID (Name) of the group to register. Group ID must be unique. Max 255 characters
Note | Arbitrary string (comment) for the Group. Max 255 characters.
Only detecting the device. | Check this if you want the group to be used only for detecting unregistered devices without allowing them to access the network. If this option is enabled, devices in the group cannot access the network even if the Network is specified in the security policy for the group.

Table 10: Displayed columns
Item Name | Description
--- | ---
Policies
Policies | List of security policies attached to the group.
Priority | A priority value of the security policy. It must be an integer in the range of 0 to 255. When multiple security policies are set, if an interface registered with a device in an UnAuth Group connects to an AMF Member, it is determined whether the security policy with the lowest priority value matches in order.
Network | ID of the network to which AMF Security assigns the device in the group.
Location | Specify a location where the device can be for AMF Security to categorize it in the group.
Schedule | Specify a schedule when the device can be connected for AMF Security to categorize it in the group.

Table 11: Buttons
Item Name | Description
--- | ---
Policies
Heading Row
Add | Open the Edit Policy dialog to add a new security policy for the UnAuth Group.
Each Row
Edit | Open the Edit Policy dialog to edit the selected security policy.
Delete | Mark to delete the security policy attached to the device. The security policy to be deleted is indicated with the DEL mark on the left side of its record line.
Revert | Clear the DEL mark on the security policy.
Page Bottom
Submit | Update the group with the input information on this page and subordinate dialogs by committing the information for the existing group.
Cancel | Cancel the operation for updating the group.

> Note

> > Interfaces and security policies marked with DEL is deleted when the "Submit" button is clicked. Once you click the "Submit" button, you cannot undo the delete operations.

#### Edit Policy

This dialog lets you add a new security policy to the group or update an existing security policy attached to the group.

Table 12: Configurable fields
Item Name | Description
--- | ---
Priority (Mandatory) | A priority value of the security policy. It must be an integer in the range of 0 to 255. When multiple security policies are set, when a device in an UnAuth Group connects to an AMF Member, it is determined whether the security policy with the lowest priority value matches in order.
Network | ID of the network which AMF Security assigns the device to. Maximum 100 IDs of the existing networks are shown in the dropdown list. If you enter text in the field, Network IDs in the dropdown list are dynamically filtered to the ones which contain the input text in Network ID, VLAN ID or Note (it shows maximum 100 elements). From the dropdown list, select a Network ID. If the registered device is connected to AMF Members, it is connected to the VLAN subnet configured in the network. If the network is not registered in the device (if this setting is blank or the VLAN ID is set to 0 in the network security policy setting), it is assigned to the VLAN set as the AMF Member. The connection to the VLAN subnet is realized by sending as a tagged VLAN with the set VLAN ID when it is sent to the upper network of the connected AMF Members. You have to add the network before assigning a device to the network. Refer to Policy Settings > Add Network for the instruction on how to register a network.
Location | Specify a location where the unauthenticated device can be so that it is categorized in the group. Maximum 100 IDs of the existing locations are shown in the dropdown list. If you enter text in the field, location IDs in the dropdown list are dynamically filtered to the ones which contain the input text in Location ID or Note (it shows maximum 100 elements). From the dropdown list, select a Location ID. If you specify Location, the UnAuth Group can access the network only from AMF Members in the location. If you do not specify Location, the UnAuth Group can access the network from all AMF Members. You have to add the location before specifying it for a group. Refer to Policy Settings > Add Location for the instructions on how to add locations.
Schedule | Specify a schedule when the unauthenticated device can be connected to the network so that it is categorized in the group. Maximum 100 IDs of the existing schedules are shown in the dropdown list. If you enter text in the field, Schedule IDs in the dropdown list are dynamically filtered to the ones which contain the input text in Schedule ID or Note (it shows maximum 100 elements). From the dropdown list, select a Schedule ID. If you specify a Schedule, the group can access the network only when the schedule is effective. If you do not specify a schedule, a device can always access the network. You have to add the schedule before specifying it for a group. Refer to Policy Settings > Add Schedule for the instruction on how to register a schedule.

> Note

> > If you can access the VLAN set for AMF Members, depending on the switch settings, the device may be able to connect to devices on the control plane.

Table 13: Buttons
Item Name | Description
--- | ---
Bottom of the dialog
Submit | Add or update the security policy information.
Cancel | Cancel the operation for adding or updating policy.

09 Jul 2021 12:05