User Guide: AMF Security mini version 2.2.0

# TCP or UDP port used by AMF Security mini

Ports AMF Security mini listens on
Packets AMF Security mini transmits

AMF Security mini uses the following port numbers internally. Please make sure that those port numbers are not used by any other processes.

## Ports AMF Security mini listens on

Services provided by AMF Security mini listen on the following ports. Listening ports can be changed for some services. But before changing them, make sure that each service port is not used by any other service.

Table 1: Listening port numbers of AMF Security services
Service Name | Port Number | Note
--- | --- | ---
Web GUI | HTTP | 80/TCP* | * Can be changed.
HTTPS | 443/TCP* | * Can be changed.
HTTP redirect service | HTTP | 80/TCP |
Internal DNS server | 53/TCP 53/UDP |
Local network name resolution service | 5355/TCP 5355/UDP |
Trap Monitor | Syslog | 514/UDP* | * Can be changed.
SNMP Trap | 162/UDP* | * Can be changed.
AMF Application Proxy Whitelist (AW+) | 1812/UDP 2083/TCP |
AMF Application Proxy Whitelist (TQ) | 1812/UDP |
Local Log Management | 9999/UDP |
Authentication Database Management | 27017/TCP |

## Packets AMF Security mini transmits

Services provided by AMF Security mini may transmit packets to the following destinations. If there are intermediate devices such as firewalls, they should be properly configured to allow those packets.

Table 2: Packets transmitted by AMF Security services
Feature | Destination | Port Number | Note
--- | --- | --- | ---
Syslog Transmission | Configured Host | 514/UDP* | * Default port.
Trap Monitor Forwarding | Syslog | Configured Host | 514/UDP* | * Default port.
SNMP | Configured Host | 162/UDP* | * Default port.
AMF Application Proxy Whitelist (AW+) | Acquisition of node information | Configured Host | 443/TCP |
AMF Application Proxy Blacklist (AW+) | Action Registration | AMF Master | 443/TCP |
State Retrieval | AMF Master | 12943/TCP |
AMF Application Proxy Whitelist (TQ) | TQ | 1812/UDP |
AMF Application Proxy Blacklist (TQ) | TQ | 1812/UDP Configured TCP port※ | ※ 5443 by default
Email Notification | Configured Host | Configured TCP port |

09 Jul 2021 12:05