User Guide: Trap Receiver version 2.5.0 for VST-VRT

# Welcome to the Trap Receiver for VST-VRT User Guide

The Trap Receiver extends Vista Manager by allowing you to monitor a wide range of third-party devices.

It is available as an optional plug-in for Vista Manager running on Vista Manager Virtual.

### Vista Manager Virtual

Vista Manager Virtual (VST-VRT) includes the tools to simplify and centralize management and security of your network. It provides an integrated graphical view for monitoring and management of wired, wireless and third-party devices.

### Vista Manager

Vista Manager is a graphical network monitoring and management tool for Allied Telesis Autonomous Management Framework™ (AMF) networks. Vista Manager automatically creates a complete topology map from an AMF network of switches, firewalls and wireless access points (APs), showing areas and multiple levels of connected nodes and devices. Vista Manager facilitates simple management of many, or all, network devices from a dashboard that gives you a central overview of your network. From the dashboard you can monitor up-to-date network status, and take action to resolve any network problems.

The Trap Receiver plug-in allows Vista Manager to also display traps received from third-party devices.

## Structure of this manual

This HTML manual covers the Trap Receiver features and how to use them. It is split into the following sections:

## Download this manual

Download a copy of this manual in ZIP format.

- User Guide: Trap Receiver version 2.5.0 for VST-VRT (download)

After downloading, extract the ZIP file and open index.html in your preferred web browser.

## Related documents

- User documents for Vista Manager Virtual (VST-VRT).

20 Sep 2021 14:30