User Guide: AWC plug-in version 3.6.0 for VST-VRT

# Initialize AWC Plug-in System

When you initialize an AWC Plug-in system, the database, the AWC Plug-in configuration, and floor map images will revert to their factory state.
Resetting the AWC Plug-in system does not affect Vista Manager EX's AMF device management information.

> Note

> > Only an Admin account can initialize the AWC Plug-in.

> Note

> > Please clear the browser cache after the initialization. If you do not clear the cache, the browser may show you the old information.

> Note

> > After you initialize and restore the AWC Plug-in system, the displayed status of an unreachable AP is the one which was last collected. Once the APs become reachable again, the latest status will be displayed.

1. Log in to Vista Manager EX using an admin account.
2. Select "System Setting" from the AWC Plug-in menu.
3. Click the "Initialize" button in the System Maintenance section.
4. The "Initialize AWC Plug-in" dialog box will appear. Click "OK".

09 Sep 2021 11:06