User Guide: AWC plug-in version 3.9.0 for VST-VRT

# Management Group

To start AP management using the AWC Plug-in, you must first create Management Groups to group APs together.
By granting access permissions for specific Management Groups to a non-admin user, administrators can permit the user to review information on a limited set of APs and AP Profiles.
By default, a single Management Group is defined, called "Default Wireless Group". Only Admins can view and edit the "Default Wireless Group".

> Note

> > The maximum number of APs that can be assigned to a single Management Group is 350.

Section 1

Table 1
Item Name | Description
--- | ---
"Create" button | Opens the "Create Management Group" dialog box. Refer to Operation Reference > Wireless Configuration > Configure Management Groups for more details.

Section 2

Table 2
Item Name | Description
--- | ---
X Group | Shows the number of Management Groups.
Search Management Group | Lets you filter the list of Management Groups. The Search field lets you enter a partial string to match. The screen displays entries with that string in one of the following fields: "Management Group Name" or "Creation Date/Time". To remove the filter, delete the string from the search field and press enter. Note The search is case-sensitive.

Section 3

Table 3: Management Group List
Item Name | Description
--- | ---
Management Group | Shows the Management Group name.
Deployed APs | Shows the number of APs in the Management Group.
AP Profiles | Shows the number of AP Profiles in the Management Group.
Deployment Maps | Shows the number of Floor Maps in the Management Group.
Createdand | Shows the date / time when the Management Group was created.
Edit (pencil icon) | Lets you edit the Management Group.
Delete (trashbin icon) | Lets you delete the Management Group. Note You cannot delete the "Default Wireless Group".

21 Oct 2022 11:59