User Guide: AT-RADGate for Allied Telesis Container Platform version 1.3.0

# Data Format

AT-RADgate policy data and system settings must be entered in a specified format. The format names and input rules frequently used for each setting are explained below.

Table 1: Format Name and Input Rule
Format Name | Input Rule
--- | ---
Identifier | The string can be up to 63 characters and can include Japanese. Spaces, tab characters, and the following symbols cannot be used. ! " # $ % & ' * + , / : ; < = > ? [ ] ^ ` `\` | { } ~
Password | You can enter alphanumeric characters and symbols within the ASCII code range.
MAC Address | This is a string that represents the MAC Address and can be entered in the following format. x is a hexadecimal number, and the case of the alphabet does not matter. xx:xx:xx:xx:xx:xx xx-xx-xx-xx-xx-xx xxxx.xxxx.xxxx xxxxxxxxxxxx
IPv4 Address | A string representing an IPv4 Address, which can be entered in the following format: n is a number between 0 and 255, and non-zero values cannot have leading zeros. n.n.n.n
Tag | Each tag is a string of up to 63 characters, with a total maximum of 255 characters. The characters that can be used are the same as those for "Identifier".

02 Apr 2026 08:03