User Guide: AMF Security Controller version 2.2.0

# Starting Configuration

Supported Web Browsers
Logging In to the Management Web Interface
Installing Licenses
Setting the timezone

## Supported Web Browsers

You can configure AMF Security through its web-based management interface.
Make sure that your management PC has one of the following web browsers installed:

- Google Chrome
- Mozilla Firefox

## Logging In to the Management Web Interface

You can configure AMF Security through its web-based management interface.

1. Start a web browser and enter the IP Address set for AMF Security.
   The IP Address is explained using 192.168.1.10.

       https://192.168.1.10

   > Note

   > > Communication between the web browser and AMF Security is over HTTPS.

2. The following login screen is displayed. Enter the default Account Name and Password and click the "Login" button.
   Entered password is masked with bullets on the screen.

   > Note

   > > The default Account Name is "manager" and the Password is "friend".

   > Note

   > > If a security warning screen appears, follow the onscreen instructions to continue browsing the site.
   > > If you have a SSL server certificate issued by a trusted certification authority (CA), you can install the certificate on the Network Settings > System Information page's or the AMF > AMF Application Proxy Settings page's "SSL Certificate" section after logging in to the AMF Security.

3. After logging in, the Device > Active Device List page is displayed.

   > Note

   > > A login session times out after 10 minutes of inactivity. The Login screen reappears when you perform any operation after the previous session has timed out.
   > > If you check "Remember this login" on the login screen, you will remain logged in.

## Installing Licenses

You have to install proper licenses before you start using AMF Security.
There are two types of licenses: "Base" and "Addon".

- You always need the Base license to run AMF Security.
  OpenFlow and AMF Application Proxy do not work until the base license is installed.
- The Addon license is for adding an OpenFlow switch. AMF Application Proxy works with a Base license only, no Addon license for nodes is required.
  Although you can install Addon licenses before installing the Base license, AMF Security does not work until the Base license is installed.

> Note

> > Purchase a license to use OpenFlow.

> Note

> > After registering the basic license, if you delete or add the basic license during operation of the OpenFlow and AMF Application Proxy network, OpenFlow and AMF Application Proxy may not operate normally.
> > Therefore, disconnect AMF security from the operating network before removing or adding a registered base license.
> > If the base license is removed or added during operation and AMF Application Proxy does not work properly, restart AMF security.

To install the license, follow the steps:

1. Click the "License page" in the message displayed at the top of the setting screen.

2. The System Settings > License page is displayed. Click the "Add" button.

3. The License dialog is displayed. Enter the "Serial Number" and "Authentication Key" shown on the license certificate and click the "Submit" button.

4. If the "Name" and "Serial Number" of the registered license are displayed on the System Settings > License page, the installation is successful.

License installation is complete. You can use AMF Security.

## Setting the timezone

For example, to use Japan time (JST: 9 hours ahead of Coordinated Universal Time (UTC)), set according to the following procedure:

> Note

> > If you change the timezone setting, AMF Security restarts. Then reboot the device.
> > Example: Open the System Settings > System Information page. Click the "Reboot" button next to "Reboot this system".
> > After that, the timezone setting is retained.

1. Click the "System Settings" menu, then click the "Date / Time Settings" submenu.

2. The System Settings > Date / Time Settings page is displayed. Click the "Edit" button in the Timezone item.

3. The Select Timezone dialog is displayed. Select the "Asia/Tokyo" from the drop-down list and click the "Submit" button.

4. Click the "OK" button.

5. After the message is displayed, AMF Security restarts and the login screen is displayed again.
   After logging in, the System Settings > Date / Time Settings page is displayed.

Timezone setting is complete.

14 Jun 2021 09:30